WDC WD2500BEVS-22UST0 FW:01.01A01 SN:WD-WXE808CF3645 (ROYL selected) port 0x8F58
Logical: Cyls 16383, Heads 16, Sectors 63, LBA 488397168, 250Gb
Controller Buffer Size: 8192Kb
Family: McKinley (Royl)

DRIVE DATA TABLES
=================
Drive Data Table Version   2
Product ID                 127A
Controller Firmware Rev.   07.38C
Overlay Firmware Revision  07.38C
Servo Firmware Revision    01.2E
Read Channel Firmware Rev. 0517260Q
Surface Format Version     A2.000

Drive Type                 3 - Mobile 2.5 Inch
Spindle Speed              5402 RPM
Area Density in Units of   125900 MB per platter

Drive Build Information
------------------------
Drive Platter Count        2
Physical HDs includ. depop 4
Virtual Heads Count        4
Heads BitMap Value         F
Zones Num                  21
Servo Wedges Num           208
RSVD Cylinders Count       128
User Cylinders Count       0
Cylinder Wedge Skew        28
Head Wedge Skew            40
Cluster Skew               68
ROM Type                   6 - Manteca
Flash Size                 192KB
Flash Programming Protocol 1
PCBA Type                  0 - Entek
PCBA Revision              0
Interface Type             2 Serial ATA

Drive Parts Information
------------------------
Controller Chip Vendor     0
Controller Chip Revision   42B1 - 
Controller Chip Family ID  44E - 
MicroP Vendor              0
MicroP Revision            42B1
Channel Chip Vendor        E6
Channel Chip Revision      11
Preamp Vendor              2
Preamp Revision            1
Power IC Vendor            0
Power IC Revision          0

Feature Flags              896
Jumper Setting Value       0 

Drive Format Information
------------------------
Tracks Per Inch            0K
Area Density               125900 per platter
Format Type                0
Drive Format Type          0 Alternate
Head Format Class          0
HDA Type (max platters num)0

SATA IPM Timers
---------------
Partial                    5 ms
Slumber                    100 ms

Error Correction Information
----------------------------
No. of Interleaves         1
OTF Corr. Span in Bytes    22
Max FW Corr. Span in Bytes 43
No. of ECC and CRC Bytes   55

ReloList File Information
-------------------------
Relocations                0
Tares                      0
Ftares                     0
Possible Remaining Relos   761
Consumed Spares            0
Last LBA of Spare Pool     1D524807

Original Drive Built Date  08-21-2008
Drive Reconfiguration Date 
MDL string                 
S/N string                 

DCM:
Spindel Motor              |
Base                       |
Latch / Crash Stop         |
Bottom VCM                 A
Media                      H
Headstack                  M
Preamp / Actuator-flex     Z
Actuator-pivot             N
Top VCM / VCM Assembly     M
Top Cover / VCM Part       R
Suspension                 F
