Please use the attached file to update Hitachi 7k1000.C (fw39C) to 3EA firmware.

Save the attached files to a DOS bootable device.
Type "JPDL_SP" enter
Select correct Hard Drive number "x"  <press enter key.>
Set new code revision => "JP0NB3EA" <press enter key.>
Select file type: 1(BDX)  <press enter key.>
Microcode start loading, monitor displays:
Drive Serial Number
Current Number of LBAs
Current Model Name
Current Microcode
New Model Name
New Microcode
Then "Pass" or "FAIL"

Please Note: their might be minor difference on the display of instruction.


от себя добавлю - действуйте согласно логике и здравому смыслу.
Я НЕ знаю, возможен ли апгрейд напрямую с 25C на 3EA.
я прошивался сначала на 39C, а затем уже заливал 3EA 
по шагам
Загружаемся в чистый DOS с любого носителя <кроме прошиваемого диска>
запускаем jpdl_sp.exe
выбираем номер винта для прошивки <из предложенного списка>
вводим номер заливаемой ревизии прошивки <3EA>
выбираем тип файла прошивки <BDX - вводим 1>
ждем несколько секунд и видим результат (PASS / FAIL)
Надеюсь что Вы увидите "PASS" ;-)