Micron 7400 NMVe SSD Firmware Update Instructions (E1MU23BC)

Date of Document: 21/October/2021 
Scope 
This document describes how to upgrade the firmware on a Micron 7400 NVMe SSD using either nvme-cli or msecli. For further assistance with this process please contact your local Micron representative. 

Upgrade using nvme-cli 
1. Download and install latest version of nvme-cli from github.com: 
	a. https://github.com/linux-nvme/nvme-cli/releases 
2. Obtain the required Micron 7400 SSD Firmware from your Micron contact or from www.micron.com: 
	a. Firmware name: E1XXXXXX 
3. List the SSDs in the system: 
	a. nvme list 
	i. Note: The target name (nvmeX) for the SSD 
4. To download the firmware, use the following nvme-cli commands: 
	a. nvme fw-download /dev/nvmeX<target> -f E1XXXXXX_release.ubi 
	i. Note: The same firmware .ubi file is used for all form factors and densities 
5. Now you need to commit the firmware, use the following nvme-cli commands: 
	a. nvme fw-commit /dev/nvmeX<target> -s 2 -a 3 
6. Confirm the firmware has been successfully updated to version E1XXXXXX 
	a. nvme list 

Upgrade using msecli 
1. Download and install latest version of msecli from micron.com: 
	a. https://www.micron.com/products/solid-state-storage/storage-executive-software 
2. Obtain the required Micron 7400 SSD Firmware from your Micron contact or from www.micron.com: 
	a. Firmware name: E1XXXXXX 
3. List the SSDs in the system: 
	a. msecli -L 
	i. Note: The target name (nvmeX) for the SSD 
4. To download the firmware, use the following msecli command: 
	a. msecli -F -U E1XXXXXX_release.ubi –n <Device Name> -S 2 
	i. Note: The same firmware .ubi file is used for all form factors and densities 
5. Confirm the firmware has been successfully updated to version E1XXXXXX 
	a. msecli -L 

Micron Technology, Inc., reserves the right to change products or specifications without notice. ©2023 Micron Technology, Inc. All rights reserved. 