Micron 9300 NVMe SSD FW Update Instructions (11300DY0)

Scope 
These instructions apply exclusively to Micron 9300 NVMe SSDs with firmware revision 11300DN0 and later.   

Firmware update 11300DY0 is applicable to all Micron 9300 SSD configurations: 

MTFDHAL3T8TDP, MTFDHAL7T6TDP, MTFDHAL15T3TDP 
MTFDHAL3T2TDR, MTFDHAL6T4TDR, MTFDHAL12T8TDR 

Firmware Update Instructions Using msecli 

Firmware update requires: 
-administrator or root user privileges
-drive with 11300DN0 or later firmware

1.Download the latest version of msecli from micron.com:
https://www.micron.com/products/solid-state-storage/storage-executive-software 

2.Firmware 11300DY0 will be provided by your Micron technical representative and is able to downgrade back to DU0.

3.List the Micron 9300 in the system to be updated:
     msecli -L 

4.Apply the update to the Micron 9300 indicated by "Device Name" using msecli:
     msecli -F -U <firmware> -n <Device_Name> 

     Windows ex: 
     msecli -F -U Micron_9300_FW-11300DY0.tar -S <FW_slot> -n      mtinvme17401955CBB6 

     Linux ex: 
     msecli -F -U Micron_9300_FW-11300DY0.tar -n /dev/nvme0 

5.Confirm the firmware has been successfully updated to version 11300DY0:
     msecli -L



Firmware Update Instructions Using nvme-cli 

Firmware update requires: 
-root user privileges
-drive with 11300DN0 or later firmware

1.Download and install latest version of nvme-cli from github.com:
https://github.com/linux-nvme/nvme-cli/releases 

2.Firmware 11300DY0 will be provided by your Micron technical representative or micron.com and is able to downgrade back to DU0.

3.List the Micron 9300 in the system to be updated:
     nvme list 

4.Apply the update to the Micron 9300 indicated by "Node" using the following nvme-cli commands:
     nvme fw-download /dev/nvme0 -f Micron_9300_FW-11300DY0.tar 

     nvme fw-commit /dev/nvme0 -s 2 -a 3

5.Confirm the firmware has been successfully updated to version 11300DY0:
     nvme id-ctrl /dev/nvme0 


Note: 

If updating from the following firmware versions: 11300B20 
 
Use conventional reset and reboot the drive/system to complete the firmware update and use command “nvme list” to confirm upgrade is completed. 


Micron Technology, Inc., reserves the right to change products or specifications without notice. ©2023 Micron Technology, Inc. All rights reserved. 