Format version = 0x0002
Версия controller firmware = 09.B2F
Версия servo firmware = 04.92
Версия overley firmware = 09.B2F
Версия surface format = A2.000
Версия read channel firmware = 03.04N28
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 3
Карта используемых головок =  0 1 2
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 180
Количество треков в SA = 96
Обороты двигателя = 5401
Количество треков в UA = 0
Cylinder skew = 28
Head skew = 40
Cluster Skew = 68
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 0Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x42B1
MicroP Vendor = 0x0000
MicroP Rev = 0x42B1
Channel Chip Vendor = 0x00E6
Channel chip Rev = 0x0011
Preamp Vendor = 0x0004
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 80Gb
Drive Format Type = 0
 
Код производителя пластин - F
Код производителя головок - G
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0004
used_heads = 0x0003
cur_capacity = 0x04B4
max_fmt_LBAs = 235302480 - 120Gb
target_capacity = 0x0001
max_target_LBAs = 234441647 - 120Gb
hq_capacity = 0x0001
max_HQ_LBAs = 235302480 - 120Gb
final_capacity = 0x0001
z0_dtpi = 0x000187B1
z0_kfci = 0x00000001
cur_svo_TPI = 0x00024DD8
cur_data_TPI_0 = 0x00023B69
cur_data_TPI_1 = 0x000228FA
cur_data_TPI_2 = 0x00021B27
cur_data_TPI_3 = 0x00000000
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x017E
cur_KFCI_1 = 0x019B
cur_KFCI_2 = 0x019B
cur_KFCI_3 = 0x0000
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 74619216 - 38Gb
max_LBA_for_head_1 = 80341632 - 41Gb
max_LBA_for_head_2 = 80341632 - 41Gb
max_LBA_for_head_3 = 0 - 0Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x00014FCE
max_user_cyls_for_head_1 = 0x000144FC
max_user_cyls_for_head_2 = 0x00013CDE
max_user_cyls_for_head_3 = 0x00000000
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0001538C
max_virt_cyls_for_head_1 = 0x00014898
max_virt_cyls_for_head_2 = 0x00014061
max_virt_cyls_for_head_3 = 0x00000000
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0080
rsvd_data_cyls = 0x0060
max_user_svo_cyls = 0x00015ABF
max_svo_cyls = 0x00015E80
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0060
trks_per_clstr_for_head_0 = 0x007C
trks_per_clstr_for_head_1 = 0x0078
trks_per_clstr_for_head_2 = 0x0075
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x02 0x03 0x04 0x00 0x00 0x00 0x00 0x00
HdMap Capacity = 0x06 0x03 0x03 0x00 0x00 0x00 0x00 0x00