Format version = 0x0002
Версия controller firmware = 02.1AC
Версия servo firmware = TM.0D
Версия overley firmware = 02.1AC
Версия surface format = B2.008
Версия read channel firmware = A1.3610H
Количество пластин = 2
Количество физических головок = 3
Количество используемых головок = 3
Карта используемых головок =  1 2 3
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 248
Количество треков в SA = 256
Обороты двигателя = 7200
Количество треков в UA = 0
Cylinder skew = 35
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 32Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7412
MicroP Vendor = 0x0000
MicroP Rev = 0x7412
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0003
Power IC vendor = 0x0000
Power IC Rev = 0x001C
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 334Gb
Drive Format Type = 0
 
Код производителя пластин - T
Код производителя головок - F
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0003
used_heads = 00003
cur_capacity = 0x9C5D
max_fmt_LBAs = 977329584 - 500Gb
target_capacity = 0x0001
max_target_LBAs = 976773167 - 500Gb
hq_capacity = 0x0001
max_HQ_LBAs = 977329584 - 500Gb
final_capacity = 0x0001
z0_dtpi = 0x0003C593
z0_kfci = 0x028F5C20
cur_svo_TPI = 0x000445C0
cur_data_TPI_0 = 0x0004B4D5
cur_data_TPI_1 = 0x00049B33
cur_data_TPI_2 = 0x000492A7
cur_data_TPI_3 = 0x00000000
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x341F
cur_KFCI_1 = 0x341F
cur_KFCI_2 = 0x341F
cur_KFCI_3 = 0x0000
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 325776528 - 166Gb
max_LBA_for_head_1 = 325776528 - 166Gb
max_LBA_for_head_2 = 325776528 - 166Gb
max_LBA_for_head_3 = 0 - 0Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x0002FC25
max_user_cyls_for_head_1 = 0x0002EB03
max_user_cyls_for_head_2 = 0x0002E45B
max_user_cyls_for_head_3 = 0x00000000
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0003016E
max_virt_cyls_for_head_1 = 0x0002F0BB
max_virt_cyls_for_head_2 = 0x0002E9F2
max_virt_cyls_for_head_3 = 0x00000000
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x0002BE85
max_svo_cyls = 0x0002C380
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x21 0x22 0x3E 0x00 0x00 0x00 0x00 0x00
HdMap Capacity = 0x11 0x11 0x11 0x00 0x00 0x00 0x00 0x00