Format version = 0x0002
Версия controller firmware = 03.CCB
Версия servo firmware = 02.C3
Версия overley firmware = 03.CCB
Версия surface format = C1.000
Версия read channel firmware = A1.3210C
Количество пластин = 3
Количество физических головок = 6
Количество используемых головок = 6
Карта используемых головок =  0 1 2 3 4 5
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 264
Количество треков в SA = 256
Обороты двигателя = 5200
Количество треков в UA = 0
Cylinder skew = 33
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 32Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7412
MicroP Vendor = 0x0000
MicroP Rev = 0x7412
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0006
Power IC vendor = 0x0000
Power IC Rev = 0x001C
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 334Gb
Drive Format Type = 3
 
Код производителя пластин - L
Код производителя головок - E
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0006
used_heads = 0x0006
cur_capacity = 0x38BD
max_fmt_LBAs = 1954680336 - 1000Gb
target_capacity = 0x0004
max_target_LBAs = 1953525167 - 1000Gb
hq_capacity = 0x0004
max_HQ_LBAs = 1954680336 - 1000Gb
final_capacity = 0x0004
z0_dtpi = 0x00038137
z0_kfci = 0x00000000
cur_svo_TPI = 0x000445C0
cur_data_TPI_0 = 0x0004DF8F
cur_data_TPI_1 = 0x00040164
cur_data_TPI_2 = 0x0004DF8F
cur_data_TPI_3 = 0x00043D34
cur_data_TPI_4 = 0x0004DF8F
cur_data_TPI_5 = 0x00045F62
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x3288
cur_KFCI_1 = 0x31C0
cur_KFCI_2 = 0x35B5
cur_KFCI_3 = 0x35B5
cur_KFCI_4 = 0x35B5
cur_KFCI_5 = 0x3356
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 315828576 - 161Gb
max_LBA_for_head_1 = 310944816 - 159Gb
max_LBA_for_head_2 = 335683152 - 171Gb
max_LBA_for_head_3 = 335683152 - 171Gb
max_LBA_for_head_4 = 335683152 - 171Gb
max_LBA_for_head_5 = 320857488 - 164Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x00033456
max_user_cyls_for_head_1 = 0x00028F6E
max_user_cyls_for_head_2 = 0x00032206
max_user_cyls_for_head_3 = 0x0002B81E
max_user_cyls_for_head_4 = 0x00031C3D
max_user_cyls_for_head_5 = 0x0002C0FD
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x00033968
max_virt_cyls_for_head_1 = 0x000293A7
max_virt_cyls_for_head_2 = 0x0003274D
max_virt_cyls_for_head_3 = 0x0002BC93
max_virt_cyls_for_head_4 = 0x0003215C
max_virt_cyls_for_head_5 = 0x0002C55E
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x0002D105
max_svo_cyls = 0x0002D580
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x03 0x42 0x2D 0x40 0x3B 0x5B 0x00 0x00
HdMap Capacity = 0x29 0x2A 0x25 0x25 0x25 0x28 0x00 0x00