Format version = 0x0002
Версия controller firmware = 05.6DG
Версия servo firmware = 01.45
Версия overley firmware = 05.6EG
Версия surface format = EX.028
Версия read channel firmware = G.00009A
Количество пластин = 4
Количество физических головок = 8
Количество используемых головок = 8
Карта используемых головок =  0 1 2 3 4 5 6 7
Тип накопителя = Enterprise 3.5 Inch
Количество зон = 21
Количество servo wedges = 368
Количество треков в SA = 256
Обороты двигателя = 7200
Количество треков в UA = 0
Cylinder skew = 29
Head skew = 120
Cluster Skew = 200
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 64Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x63B0
MicroP Vendor = 0x0000
MicroP Rev = 0x63B0
Channel Chip Vendor = 0x0009
Channel chip Rev = 0x0020
Preamp Vendor = 0x0000
Preamp Rev = 0x0003
Power IC vendor = 0x0000
Power IC Rev = 0x2100
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 42
No. of ecc bytes in read/write long sector = 80
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 502Gb
Drive Format Type = 1
 
Код производителя пластин - W
Код производителя головок - T
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0008
used_heads = 0x0008
cur_capacity = 0x4E24
max_fmt_LBAs = 3908273040 - 2001Gb
target_capacity = 0x0002
max_target_LBAs = 3907029167 - 2000Gb
hq_capacity = 0x0002
max_HQ_LBAs = 3908273040 - 2001Gb
final_capacity = 0x0002
z0_dtpi = 0x0003665C
z0_kfci = 0x00000014
cur_svo_TPI = 0x00038270
cur_data_TPI_0 = 0x0003EBB9
cur_data_TPI_1 = 0x0003C8A0
cur_data_TPI_2 = 0x0003C8A0
cur_data_TPI_3 = 0x0003C8A0
cur_data_TPI_4 = 0x0003A588
cur_data_TPI_5 = 0x0003E4B4
cur_data_TPI_6 = 0x0003E4B4
cur_data_TPI_7 = 0x0003E4B4
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x09C4
cur_KFCI_1 = 0x09C4
cur_KFCI_2 = 0x09C4
cur_KFCI_3 = 0x09C4
cur_KFCI_4 = 0x0A05
cur_KFCI_5 = 0x0987
cur_KFCI_6 = 0x09C4
cur_KFCI_7 = 0x09C4
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 488463696 - 250Gb
max_LBA_for_head_1 = 488463696 - 250Gb
max_LBA_for_head_2 = 488463696 - 250Gb
max_LBA_for_head_3 = 488463696 - 250Gb
max_LBA_for_head_4 = 501085872 - 256Gb
max_LBA_for_head_5 = 476404992 - 243Gb
max_LBA_for_head_6 = 488463696 - 250Gb
max_LBA_for_head_7 = 488463696 - 250Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x0003E4F6
max_user_cyls_for_head_1 = 0x0003BBAD
max_user_cyls_for_head_2 = 0x0003B234
max_user_cyls_for_head_3 = 0x0003B234
max_user_cyls_for_head_4 = 0x00039BC6
max_user_cyls_for_head_5 = 0x0003D1D0
max_user_cyls_for_head_6 = 0x0003D1C0
max_user_cyls_for_head_7 = 0x0003D1BA
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0003EB1B
max_virt_cyls_for_head_1 = 0x0003C18A
max_virt_cyls_for_head_2 = 0x0003B7F9
max_virt_cyls_for_head_3 = 0x0003B7F9
max_virt_cyls_for_head_4 = 0x0003A173
max_virt_cyls_for_head_5 = 0x0003D7C5
max_virt_cyls_for_head_6 = 0x0003D7B0
max_virt_cyls_for_head_7 = 0x0003D7B0
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x00039177
max_svo_cyls = 0x00039780
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x11 0x19 0x20 0x20 0x1A 0x1F 0x1F 0x1F
HdMap Capacity = 0x04 0x04 0x04 0x04 0x03 0x05 0x04 0x04