Format version = 0x0002
Версия controller firmware = 02.C0E
Версия servo firmware = 03.09
Версия overley firmware = 02.C0E
Версия surface format = A1.002
Версия read channel firmware = 0914345S
Количество пластин = 1
Количество физических головок = 2
Количество используемых головок = 2
Карта используемых головок = 0 1
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 276
Количество треков в SA = 170
Обороты двигателя = 7200
Количество треков в UA = 0
Cylinder skew = 40
Head skew = 77
Cluster Skew = 130
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Parallel ATA
Установленная память = 8Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x46A1
MicroP Vendor = 0x0000
MicroP Rev = 0x46A1
Channel Chip Vendor = 0x0058
Channel chip Rev = 0x0020
Preamp Vendor = 0x0000
Preamp Rev = 0x0005
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density in units of 100MB per platter = 3207
Drive Format Type = 0