Format version = 0x0002
Версия controller firmware = 21.1FM
Версия servo firmware = 00.19
Версия overley firmware = 21.1FM
Версия surface format = A2.01E
Версия read channel firmware = 01.12M  
Количество пластин = 3
Количество физических головок = 6
Количество используемых головок = 6
Карта используемых головок = 0 1 2 3 4 5
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 216
Количество треков в SA = 64
Обороты двигателя = 7204
Количество треков в UA = 103520
Cylinder skew = 24
Head skew = 55
Cluster Skew = 89
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 0Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x31B2
MicroP Vendor = 0x0000
MicroP Rev = 0x31B2
Channel Chip Vendor = 0x0046
Channel chip Rev = 0x0021
Preamp Vendor = 0x0000
Preamp Rev = 0x0000
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 50
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 107Gb
Drive Format Type = 0