Format version = 0x0002
Версия controller firmware = 07.FTC
Версия servo firmware = 01.E7
Версия overley firmware = 07.FTC
Версия surface format = C2.007
Версия read channel firmware = 0528300S
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 4
Карта используемых головок =  0 1 2 3
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 208
Количество треков в SA = 256
Обороты двигателя = 7211
Количество треков в UA = 0
Cylinder skew = 40
Head skew = 90
Cluster Skew = 130
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 16Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x45D0
MicroP Vendor = 0x0000
MicroP Rev = 0x45D0
Channel Chip Vendor = 0x0058
Channel chip Rev = 0x0001
Preamp Vendor = 0x0001
Preamp Rev = 0x0002
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 161Gb
Drive Format Type = 0
 
Код производителя пластин - L
Код производителя головок - I
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0004
used_heads = 0x0004
cur_capacity = 0x0C80
max_fmt_LBAs = 625470048 - 320Gb
target_capacity = 0x0001
max_target_LBAs = 625142447 - 320Gb
hq_capacity = 0x0001
max_HQ_LBAs = 625470048 - 320Gb
final_capacity = 0x0001
z0_dtpi = 0x0002B1B2
z0_kfci = 0x00000003
cur_svo_TPI = 0x00030D40
cur_data_TPI_0 = 0x0002D651
cur_data_TPI_1 = 0x0002EEBB
cur_data_TPI_2 = 0x0002EEBB
cur_data_TPI_3 = 0x0002CA1C
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x0320
cur_KFCI_1 = 0x030C
cur_KFCI_2 = 0x0334
cur_KFCI_3 = 0x0320
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 156353904 - 80Gb
max_LBA_for_head_1 = 152445888 - 78Gb
max_LBA_for_head_2 = 160316352 - 82Gb
max_LBA_for_head_3 = 156353904 - 80Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x0001B56C
max_user_cyls_for_head_1 = 0x0001D29E
max_user_cyls_for_head_2 = 0x0001CC51
max_user_cyls_for_head_3 = 0x0001B9E7
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0001B815
max_virt_cyls_for_head_1 = 0x0001D5FB
max_virt_cyls_for_head_2 = 0x0001D051
max_virt_cyls_for_head_3 = 0x0001BDD9
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x0001E878
max_svo_cyls = 0x0001ED00
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x44 0x07 0x1B 0x09 0x00 0x00 0x00 0x00
HdMap Capacity = 0x0B 0x0C 0x0A 0x0B 0x00 0x00 0x00 0x00