Analysing Flash.bin ...

Searching for LDSCs and verifying PCMBlocks ...

LDSC   LDSC    Att   PCMBlock          RAM         size      PCMBlk CS
Start  ID CS        Start -  End     address     RAM / ROM    Exp/Act
-----  -- --   --   -----   -----   --------   ------ -----  ---------
    0  5A 03   04     120 -   CC4      10C00      BA4   BA4    5F   5F   OK
   20  01 C8   01     CC5 -  7641          0 c   83A0  697C    04   04   OK
   40  02 46   01    7642 -  B766       854C c   5C8C  4124    5A   5A   OK
   60  03 7B   01    B767 -  BF47       E6C8 c    9CC   7E0    37   37   OK
   80  04 92   03    BF48 -  C118    4000064 c    270   1D0    E4   E4   OK
   A0  05 03   03    C119 -  C64D    40041AC c    AAC   534    76   76   OK
   C0  06 43   03    C64E -  DCB6   24000000 c   26D8  1668    A8   A8   OK
   E0  07 AA   00    DCB7 - 2598F   FFE17E00    17CD8 17CD8    79   79   OK
  100  08 19   01   25990 - 2BBD8   FFE30200 c   7D64  6248    0A   0A   OK

LDSC   = PM Loader Config String (32 bytes)
ID     = ID byte of LDSC (byte #0)
CS     = Checksum byte or word
Att    = Attributes
PCMBlk = Program Code Memory Block
Exp    = Expected checksum for PCMBLock
Act    = Actual checksum for PCMBLock
c      = compressed PCMBlock
size   = size of decompressed (in RAM) and compressed (in ROM) PCMBlock in bytes


ROYL directory module 0x000B found at 0x2FEE1

Active directory flag = 0x00

Identifying SA regions ...

Reg#    Reg size     Reg loc
----  ----------  ----------
0x00  0x0000C90F  0x00000000
0x01  0x0000C90F  0x0001AC7F

Verifying ROYL modules ...

 ID          Size (bytes)         Address    Checksum
 dir   hdr        dir       hdr
----  ----   --------  --------   --------   --------
000A  OK     0000003E  00000200   0002FFB2   00000000  OK
000B  OK     000000D1  00000200   0002FEE1   00000000  OK
0030  OK     00000400  OK         0002FAE1   00000000  OK
0047  OK     00000400  OK         0002F348   00000000  OK
000D  OK     00000046  00000200   0002F302   00000000  OK
004F  OK     000000B8  00000200   0002F748   00000000  OK

dir  -  Module ID/Size as reported in directory module (0x20B or 0x0B)
hdr  -  Module ID/Size as reported in module's header
N/A  -  Not Applicable
BAD  -  Module has invalid checksum. This may be due to non-existent module.

ROM modules saved to Flash_00\000Bmods and Flash_00\020Bmods

Active directory is 0x0B -- directory 0x20B not present

Analysing active 0x0A module ...

Head map checksum (Expected / Actual) = 0x0000 / 0x0000 - OK
Number of heads (physical / in use) = 2/2
Head map #1 = 0x03 / 0b00000011
Head map #2 = 0x03 / 0b00000011

Analysing active 0x0D module ...

Firmware Version = 58.01D58
World Wide Name = 50014EE1562B3837


Analysing active 0x4F module ...

ROM version = 005800A6

Analysing active 0x47 module ...

Preamp values
-----------
0  0B05B10F
1  0B06B10F
2  550AA10C
3  550AA10C
4  550AA10C
5  550AA10C
6  550AA10C
7  550AA10C

Microjogs
-------
0  0A9A
1  0A02
2  0670
3  0670
4  0670
5  0670
6  0670
7  0670

Head/Media DCM = 7K
