Format version = 0x0002
Версия controller firmware = 20.0PD
Версия servo firmware = 0B.36
Версия overley firmware = 20.0QD
Версия surface format = C1.007
Версия read channel firmware = AA01JJ38
Количество пластин = 3
Количество физических головок = 6
Количество используемых головок = 5
Карта используемых головок = 1 2 5 6 7
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 396
Количество треков в SA = 256
Обороты двигателя = 5000
Количество треков в UA = 0
Cylinder skew = 55
Head skew = 77
Cluster Skew = 130
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 64Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7412
MicroP Vendor = 0x0000
MicroP Rev = 0x7412
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x2100
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 673Gb
Drive Format Type = 0