Format version = 0x0002
Версия controller firmware = 01.5MA
Версия servo firmware = 02.B2
Версия overley firmware = 01.5NA
Версия surface format = C1.A02
Версия read channel firmware = n017419T
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 1
Карта используемых головок = 2
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 288
Количество треков в SA = 256
Обороты двигателя = 7200
Количество треков в UA = 0
Cylinder skew = 42
Head skew = 77
Cluster Skew = 130
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 32Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x63B0
MicroP Vendor = 0x0000
MicroP Rev = 0x63B0
Channel Chip Vendor = 0x0009
Channel chip Rev = 0x0020
Preamp Vendor = 0x0001
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x2100
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 42
No. of ecc bytes in read/write long sector = 75
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 500Gb
Drive Format Type = 0
 
Код производителя пластин - K
Код производителя головок - 7
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0002
cur_stroke = 0x0001
phy_heads = 0x0004
used_heads = 00003
cur_capacity = 0x2819
max_fmt_LBAs = 1491155568 - 763Gb
target_capacity = 0x0001
max_target_LBAs = 1953525167 - 1000Gb
hq_capacity = 0x0001
max_HQ_LBAs = 1491155568 - 763Gb
final_capacity = 0x0001
z0_dtpi = 0x0002C5FD
z0_kfci = 0x00000006
cur_svo_TPI = 0x000395F8
cur_data_TPI_0 = 0x00039D23
cur_data_TPI_1 = 0x0003D683
cur_data_TPI_2 = 0x0003D683
cur_data_TPI_3 = 0x00000000
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x09C4
cur_KFCI_1 = 0x09C5
cur_KFCI_2 = 0x0A48
cur_KFCI_3 = 0x0000
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 488409264 - 250Gb
max_LBA_for_head_1 = 488595744 - 250Gb
max_LBA_for_head_2 = 514150560 - 263Gb
max_LBA_for_head_3 = 0 - 0Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x00038F2B
max_user_cyls_for_head_1 = 0x0003CC2B
max_user_cyls_for_head_2 = 0x0003B7A7
max_user_cyls_for_head_3 = 0x00000000
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0003AF24
max_virt_cyls_for_head_1 = 0x0003EEFA
max_virt_cyls_for_head_2 = 0x0003D880
max_virt_cyls_for_head_3 = 0x00000000
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x00039704
max_svo_cyls = 0x0003B780
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x05 0x03 0x17 0x17 0x00 0x00 0x00 0x00
HdMap Capacity = 0x04 0x04 0x02 0x02 0x00 0x00 0x00 0x00