Format version = 0x0002
Версия controller firmware = 08.0WA
Версия servo firmware = 01.11
Версия overley firmware = 08.0WA
Версия surface format = M3.201
Версия read channel firmware = 0128008S
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 4
Карта используемых головок = 0 1 2 3
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 208
Количество треков в SA = 128
Обороты двигателя = 5406
Количество треков в UA = 0
Cylinder skew = 28
Head skew = 40
Cluster Skew = 68
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 8Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x42B1
MicroP Vendor = 0x0000
MicroP Rev = 0x42B1
Channel Chip Vendor = 0x00E6
Channel chip Rev = 0x0011
Preamp Vendor = 0x0002
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 160Gb
Drive Format Type = 0