The default batch files are set to boards B3 Firmware, when running 1_ListAllAdaptors.sh
check to make sure your board is not a B2,
if so you will need to update the batch files to point to the B2 firmware version.
