Format version = 0x0002
Версия controller firmware = 05.F0E
Версия servo firmware = 04.AL
Версия overley firmware = 05.F0E
Версия surface format = EX.013
Версия read channel firmware = 0914349S
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 4
Карта используемых головок =  0 1 2 3
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 276
Количество треков в SA = 170
Обороты двигателя = 7200
Количество треков в UA = 0
Cylinder skew = 25
Head skew = 77
Cluster Skew = 130
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 16Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x46A1
MicroP Vendor = 0x0000
MicroP Rev = 0x46A1
Channel Chip Vendor = 0x0058
Channel chip Rev = 0x0020
Preamp Vendor = 0x0000
Preamp Rev = 0x0002
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 320Gb
Drive Format Type = 0
 
Код производителя пластин - K
Код производителя головок - 6
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0004
used_heads = 0x0004
cur_capacity = 0x1901
max_fmt_LBAs = 1250596368 - 640Gb
target_capacity = 0x0001
max_target_LBAs = 1250263727 - 640Gb
hq_capacity = 0x0001
max_HQ_LBAs = 1250596368 - 640Gb
final_capacity = 0x0001
z0_dtpi = 0x00029718
z0_kfci = 0x00000004
cur_svo_TPI = 0x00032858
cur_data_TPI_0 = 0x0002C99D
cur_data_TPI_1 = 0x0002B05A
cur_data_TPI_2 = 0x0002C99D
cur_data_TPI_3 = 0x0002B05A
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x0669
cur_KFCI_1 = 0x0618
cur_KFCI_2 = 0x0640
cur_KFCI_3 = 0x0640
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 320596416 - 164Gb
max_LBA_for_head_1 = 304836336 - 156Gb
max_LBA_for_head_2 = 312581808 - 160Gb
max_LBA_for_head_3 = 312581808 - 160Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x0002CADB
max_user_cyls_for_head_1 = 0x0002B193
max_user_cyls_for_head_2 = 0x0002CADB
max_user_cyls_for_head_3 = 0x0002B18E
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0002CCD8
max_virt_cyls_for_head_1 = 0x0002B378
max_virt_cyls_for_head_2 = 0x0002CCD8
max_virt_cyls_for_head_3 = 0x0002B378
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0100
rsvd_data_cyls = 0x00AA
max_user_svo_cyls = 0x000328F7
max_svo_cyls = 0x00032C00
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x00AA
trks_per_clstr_for_head_0 = 0x0071
trks_per_clstr_for_head_1 = 0x006D
trks_per_clstr_for_head_2 = 0x0071
trks_per_clstr_for_head_3 = 0x006D
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x05 0x06 0x05 0x06 0x00 0x00 0x00 0x00
HdMap Capacity = 0x0A 0x0C 0x0B 0x0B 0x00 0x00 0x00 0x00