Format version = 0x0002
Версия controller firmware = 65.43V
Версия servo firmware = 05.0B
Версия overley firmware = 65.43V
Версия surface format = A1.001
Версия read channel firmware = G.00001A
Количество пластин = 1
Количество физических головок = 2
Количество используемых головок = 2
Карта используемых головок = 0 1
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 248
Количество треков в SA = 256
Обороты двигателя = 5400
Количество треков в UA = 0
Cylinder skew = 33
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 16Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7412
MicroP Vendor = 0x0000
MicroP Rev = 0x7412
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0000
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 321Gb
Drive Format Type = 0
 
Код производителя пластин - L
Код производителя головок - W
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0002
used_heads = 00002
cur_capacity = 0x640E
max_fmt_LBAs = 625363200 - 320Gb
target_capacity = 0x0001
max_target_LBAs = 625142447 - 320Gb
hq_capacity = 0x0001
max_HQ_LBAs = 625363200 - 320Gb
final_capacity = 0x0001
z0_dtpi = 0x0003E7C1
z0_kfci = 0x028F5C1A
cur_svo_TPI = 0x000445C0
cur_data_TPI_0 = 0x00047905
cur_data_TPI_1 = 0x000445C0
cur_data_TPI_2 = 0x00000000
cur_data_TPI_3 = 0x00000000
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x3207
cur_KFCI_1 = 0x3207
cur_KFCI_2 = 0x0000
cur_KFCI_3 = 0x0000
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 312681600 - 160Gb
max_LBA_for_head_1 = 312681600 - 160Gb
max_LBA_for_head_2 = 0 - 0Gb
max_LBA_for_head_3 = 0 - 0Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x0002CD73
max_user_cyls_for_head_1 = 0x0002A650
max_user_cyls_for_head_2 = 0x00000000
max_user_cyls_for_head_3 = 0x00000000
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0002D206
max_virt_cyls_for_head_1 = 0x0002AA86
max_virt_cyls_for_head_2 = 0x00000000
max_virt_cyls_for_head_3 = 0x00000000
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x0002B777
max_svo_cyls = 0x0002BC00
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x16 0x34 0x00 0x00 0x00 0x00 0x00 0x00
HdMap Capacity = 0x06 0x06 0x00 0x00 0x00 0x00 0x00 0x00