Format version = 0x0002
Версия controller firmware = 14.39T
Версия servo firmware = 05.1C
Версия overley firmware = 14.39T
Версия surface format = D1.000
Версия read channel firmware = AA01H400
Количество пластин = 1
Количество физических головок = 2
Количество используемых головок = 2
Карта используемых головок =  0 1
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 248
Количество треков в SA = 256
Обороты двигателя = 5400
Количество треков в UA = 0
Cylinder skew = 31
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 8Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x63B0
MicroP Vendor = 0x0000
MicroP Rev = 0x63B0
Channel Chip Vendor = 0x0009
Channel chip Rev = 0x0020
Preamp Vendor = 0x0001
Preamp Rev = 0x0000
Power IC vendor = 0x0000
Power IC Rev = 0x001C
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 45
No. of ecc bytes in read/write long sector = 75
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 321Gb
Drive Format Type = 0
 
Код производителя пластин - T
Код производителя головок - G
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0002
used_heads = 0x0002
cur_capacity = 0x0C80
max_fmt_LBAs = 625248288 - 320Gb
target_capacity = 0x0000
max_target_LBAs = 0 - 0Gb
hq_capacity = 0x0000
max_HQ_LBAs = 625248288 - 320Gb
final_capacity = 0x0000
z0_dtpi = 0x0003E7C1
z0_kfci = 0x00000002
cur_svo_TPI = 0x000445C0
cur_data_TPI_0 = 0x00051B5F
cur_data_TPI_1 = 0x00051B5F
cur_data_TPI_2 = 0x00000000
cur_data_TPI_3 = 0x00000000
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x0640
cur_KFCI_1 = 0x0640
cur_KFCI_2 = 0x0000
cur_KFCI_3 = 0x0000
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 312624144 - 160Gb
max_LBA_for_head_1 = 312624144 - 160Gb
max_LBA_for_head_2 = 0 - 0Gb
max_LBA_for_head_3 = 0 - 0Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x00033471
max_user_cyls_for_head_1 = 0x0003346A
max_user_cyls_for_head_2 = 0x00000000
max_user_cyls_for_head_3 = 0x00000000
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x000339A6
max_virt_cyls_for_head_1 = 0x000339A6
max_virt_cyls_for_head_2 = 0x00000000
max_virt_cyls_for_head_3 = 0x00000000
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x0002B777
max_svo_cyls = 0x0002BC00
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x0F 0x0F 0x00 0x00 0x00 0x00 0x00 0x00
HdMap Capacity = 0x04 0x04 0x00 0x00 0x00 0x00 0x00 0x00