Format version = 0x0002
Версия controller firmware = 14.D9R
Версия servo firmware = 05.CM
Версия overley firmware = 14.D9R
Версия surface format = EX.048
Версия read channel firmware = AA01A04F
Количество пластин = 1
Количество физических головок = 2
Количество используемых головок = 2
Карта используемых головок = 0 1
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 248
Количество треков в SA = 256
Обороты двигателя = 5400
Количество треков в UA = 0
Cylinder skew = 31
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 8Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x63A1
MicroP Vendor = 0x0000
MicroP Rev = 0x63A1
Channel Chip Vendor = 0x0009
Channel chip Rev = 0x0011
Preamp Vendor = 0x0001
Preamp Rev = 0x0000
Power IC vendor = 0x0000
Power IC Rev = 0x0018
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 42
No. of ecc bytes in read/write long sector = 75
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 320Gb
Drive Format Type = 0