Format version = 0x0002
Версия controller firmware = 16.0FW
Версия servo firmware = 07.12
Версия overley firmware = 16.0FW
Версия surface format = W1.001
Версия read channel firmware = AA01H41D
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 4
Карта используемых головок =  0 1 2 3
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 248
Количество треков в SA = 256
Обороты двигателя = 5400
Количество треков в UA = 0
Cylinder skew = 31
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 8Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x63B0
MicroP Vendor = 0x0000
MicroP Rev = 0x63B0
Channel Chip Vendor = 0x0009
Channel chip Rev = 0x0020
Preamp Vendor = 0x0001
Preamp Rev = 0x0003
Power IC vendor = 0x0000
Power IC Rev = 0x001C
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 45
No. of ecc bytes in read/write long sector = 75
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 251Gb
Drive Format Type = 1
 
Код производителя пластин - H
Код производителя головок - P
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0004
used_heads = 0x0004
cur_capacity = 0x1388
max_fmt_LBAs = 976961664 - 500Gb
target_capacity = 0x0002
max_target_LBAs = 976773167 - 500Gb
hq_capacity = 0x0002
max_HQ_LBAs = 976961664 - 500Gb
final_capacity = 0x0002
z0_dtpi = 0x00031926
z0_kfci = 0x00000005
cur_svo_TPI = 0x00038270
cur_data_TPI_0 = 0x0003BA97
cur_data_TPI_1 = 0x0003BA97
cur_data_TPI_2 = 0x00039E83
cur_data_TPI_3 = 0x00039E83
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x04E2
cur_KFCI_1 = 0x04E2
cur_KFCI_2 = 0x04E2
cur_KFCI_3 = 0x04E2
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 244240416 - 125Gb
max_LBA_for_head_1 = 244240416 - 125Gb
max_LBA_for_head_2 = 244240416 - 125Gb
max_LBA_for_head_3 = 244240416 - 125Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x000251C8
max_user_cyls_for_head_1 = 0x00025142
max_user_cyls_for_head_2 = 0x0002431D
max_user_cyls_for_head_3 = 0x0002498C
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x000255BA
max_virt_cyls_for_head_1 = 0x000255BA
max_virt_cyls_for_head_2 = 0x00024795
max_virt_cyls_for_head_3 = 0x00024E1F
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x00023A85
max_svo_cyls = 0x00023E80
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x23 0x23 0x1A 0x10 0x00 0x00 0x00 0x00
HdMap Capacity = 0x04 0x04 0x04 0x04 0x00 0x00 0x00 0x00