Cur stroke: 1                                

Phy heads: 4                                 

Used heads: 3                                

Cur capacity: 2505                           

Final capacity_selection: 1                  

Max fmt LBAs: 489530160 = 233,43 Gb          

Target capacity selection: 1                 

Target max_fmt LBAs: 488397167 = 232,89 Gb   

Hq capacity selection: 1                     

HQ max fmt LBAs: 489530160 = 233,43 Gb       

Reserved1: 0                                 

Reserved2: 0                                 

Reserved3: 0                                 

Reserved4: 0                                 



Zone 0 DTPI: 176562                          

Zone 0 KFCI: 2                               

Cur svo TPI: 200000                          

Cur_data_TPI_0: 196875                       

Cur_data_TPI_1: 187500                       

Cur_data_TPI_2: 196875                       

Cur_data_TPI_3: 0                            

Cur_data_TPI_4: 0                            

Cur_data_TPI_5: 0                            

Cur_data_TPI_6: 0                            

Cur_data_TPI_7: 0                            





Cur_KFCI_0: 901                              

Cur_KFCI_1: 792                              

Cur_KFCI_2: 812                              

Cur_KFCI_3: 0                                

Cur_KFCI_4: 0                                

Cur_KFCI_5: 0                                

Cur_KFCI_6: 0                                

Cur_KFCI_7: 0                                

Cur_KFCI_8: 0                                

Cur KFCI 9: 0                                





Max_LBA_for_head_0: 176048208 = 83,95 Gb     

Max_LBA_for_head_1: 154708848 = 73,77 Gb     

Max_LBA_for_head_2: 158773104 = 75,71 Gb     

Max_LBA_for_head_3: 0 = 0,00 Gb              

Max_LBA_for_head_4: 0 = 0,00 Gb              

Max_LBA_for_head_5: 0 = 0,00 Gb              

Max_LBA_for_head_6: 0 = 0,00 Gb              

Max_LBA_for_head_7: 0 = 0,00 Gb              





Max_user_cyls_for_head_0: 121658             

Max_user_cyls_for_head_1: 114983             

Max_user_cyls_for_head_2: 117556             

Max_user_cyls_for_head_3: 0                  

Max_user_cyls_for_head_4: 0                  

Max_user_cyls_for_head_5: 0                  

Max_user_cyls_for_head_6: 0                  

Max_user_cyls_for_head_7: 0                  





Max_virt_cyls_for_head_0: 122616             

Max_virt_cyls_for_head_1: 115904             

Max_virt_cyls_for_head_2: 118536             

Max_virt_cyls_for_head_3: 0                  

Max_virt_cyls_for_head_4: 0                  

Max_virt_cyls_for_head_5: 0                  

Max_virt_cyls_for_head_6: 0                  

Max_virt_cyls_for_head_7: 0                  





Rsvd_svo_cyls: 512                           

Rsvd_data_cyls: 256                          

Trks_per_clstr_svo: 128                      

Trks_per_clstr_rsvd: 0                       





Trks_per_clstr_for_head_0: 0                 

Trks_per_clstr_for_head_1: 0                 

Trks_per_clstr_for_head_2: 0                 

Trks_per_clstr_for_head_3: 0                 

Trks_per_clstr_for_head_4: 0                 

Trks_per_clstr_for_head_5: 0                 

Trks_per_clstr_for_head_6: 0                 

Trks_per_clstr_for_head_7: 0                 





Stroke = 1                                   

DCM = 1                                      

Pad4 = 00000000000000000000                  

hq_KFCI_0 = 901                              

hq_KFCI_1 = 792                              

hq_KFCI_2 = 812                              

hq_KFCI_3 = 0                                

hq_KFCI_4 = 0                                

hq_KFCI_5 = 0                                

hq_KFCI_6 = 0                                

hq_KFCI_7 = 0                                

dtpi_selection = 29376                       

kfci_selection = 1377                        

Cur_TPI  Hd0  = 16                           

Cur_KFCI  Hd0 = 1                            

Cur_TPI  Hd1  = 28                           

Cur_KFCI  Hd1 = 6                            

Cur_TPI  Hd2  = 66                           

Cur_KFCI  Hd2 = 5                            

Cur_TPI  Hd3  = 0                            

Cur_KFCI  Hd3 = 0                            

Cur_TPI  Hd4  = 0                            

Cur_KFCI  Hd4 = 0                            

Cur_TPI  Hd5  = 0                            

Cur_KFCI  Hd5 = 0                            

Cur_TPI  Hd6  = 0                            

Cur_KFCI  Hd6 = 0                            

Cur_TPI  Hd7  = 0                            

Cur_KFCI  Hd7 = 0                            


