Format version = 0x0002
Версия controller firmware = 20.0AB
Версия servo firmware = 0B.21
Версия overley firmware = 20.0BB
Версия surface format = C1.005
Версия read channel firmware = AA01Jj37
Количество пластин = 3
Количество физических головок = 6
Количество используемых головок = 6
Карта используемых головок =  0 1 2 5 6 7
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 396
Количество треков в SA = 256
Обороты двигателя = 5000
Количество треков в UA = 0
Cylinder skew = 55
Head skew = 77
Cluster Skew = 130
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 64Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7411
MicroP Vendor = 0x0000
MicroP Rev = 0x7411
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x2100
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 670Gb
Drive Format Type = 0
 
Код производителя пластин - K
Код производителя головок - 6
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0006
used_heads = 00006
cur_capacity = 0x724F
max_fmt_LBAs = 3914493408 - 2004Gb
target_capacity = 0x0001
max_target_LBAs = 3907029167 - 2000Gb
hq_capacity = 0x0001
max_HQ_LBAs = 3914493408 - 2004Gb
final_capacity = 0x0001
z0_dtpi = 0x00037180
z0_kfci = 0x028F5C24
cur_svo_TPI = 0x00040B28
cur_data_TPI_0 = 0x00040311
cur_data_TPI_1 = 0x00042B81
cur_data_TPI_2 = 0x00046C33
cur_data_TPI_3 = 0x00042B81
cur_data_TPI_4 = 0x0003DAA2
cur_data_TPI_5 = 0x0003E2B8
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x65BB
cur_KFCI_1 = 0x6B00
cur_KFCI_2 = 0x6850
cur_KFCI_3 = 0x6DCE
cur_KFCI_4 = 0x65BB
cur_KFCI_5 = 0x65BB
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 635824224 - 325Gb
max_LBA_for_head_1 = 668753568 - 342Gb
max_LBA_for_head_2 = 651969360 - 333Gb
max_LBA_for_head_3 = 686297808 - 351Gb
max_LBA_for_head_4 = 635824224 - 325Gb
max_LBA_for_head_5 = 635824224 - 325Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x0003F218
max_user_cyls_for_head_1 = 0x00040CA4
max_user_cyls_for_head_2 = 0x00043EF2
max_user_cyls_for_head_3 = 0x000428A3
max_user_cyls_for_head_4 = 0x0003B447
max_user_cyls_for_head_5 = 0x0003BD34
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x0003FCB3
max_virt_cyls_for_head_1 = 0x00041756
max_virt_cyls_for_head_2 = 0x000449D2
max_virt_cyls_for_head_3 = 0x0004342A
max_virt_cyls_for_head_4 = 0x0003BE90
max_virt_cyls_for_head_5 = 0x0003C7C4
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x00041D78
max_svo_cyls = 0x00042900
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x1D 0x27 0x3B 0x06 0x3F 0x34 0x00 0x00
HdMap Capacity = 0x05 0x03 0x04 0x02 0x05 0x05 0x00 0x00