Format version = 0x0002
Версия controller firmware = 20.76E
Версия servo firmware = 0B.3B
Версия overley firmware = 20.77E
Версия surface format = C1.A16
Версия read channel firmware = G.00001A
Количество пластин = 3
Количество физических головок = 6
Количество используемых головок = 5
Карта используемых головок =  0 1 2 6 7
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 396
Количество треков в SA = 256
Обороты двигателя = 5000
Количество треков в UA = 0
Cylinder skew = 55
Head skew = 77
Cluster Skew = 130
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 64Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7411
MicroP Vendor = 0x0000
MicroP Rev = 0x7411
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x2100
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 600Gb
Drive Format Type = 0
 
Код производителя пластин - K
Код производителя головок - 9
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0006
used_heads = 00005
cur_capacity = 0x77DA
max_fmt_LBAs = 3329168976 - 1704Gb
target_capacity = 0x0001
max_target_LBAs = 3907029167 - 2000Gb
hq_capacity = 0x0001
max_HQ_LBAs = 3329168976 - 1704Gb
final_capacity = 0x0001
z0_dtpi = 0x00037180
z0_kfci = 0x028F5C24
cur_svo_TPI = 0x00040B28
cur_data_TPI_0 = 0x00044BDA
cur_data_TPI_1 = 0x00040311
cur_data_TPI_2 = 0x000494A3
cur_data_TPI_3 = 0x00044BDA
cur_data_TPI_4 = 0x00044BDA
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x6C5B
cur_KFCI_1 = 0x6A86
cur_KFCI_2 = 0x6C61
cur_KFCI_3 = 0x6E31
cur_KFCI_4 = 0x6335
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 677240928 - 346Gb
max_LBA_for_head_1 = 665782992 - 340Gb
max_LBA_for_head_2 = 677383056 - 346Gb
max_LBA_for_head_3 = 688707936 - 352Gb
max_LBA_for_head_4 = 620054064 - 317Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x000386A6
max_user_cyls_for_head_1 = 0x00033EDB
max_user_cyls_for_head_2 = 0x0003B243
max_user_cyls_for_head_3 = 0x000385C8
max_user_cyls_for_head_4 = 0x00038588
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x00044E55
max_virt_cyls_for_head_1 = 0x0003F3D7
max_virt_cyls_for_head_2 = 0x000481B3
max_virt_cyls_for_head_3 = 0x00044E9D
max_virt_cyls_for_head_4 = 0x00044E6F
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0200
rsvd_data_cyls = 0x0100
max_user_svo_cyls = 0x00036678
max_svo_cyls = 0x00042900
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0000
trks_per_clstr_for_head_0 = 0x0000
trks_per_clstr_for_head_1 = 0x0000
trks_per_clstr_for_head_2 = 0x0000
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x10 0x28 0x24 0x10 0x10 0x10 0x00 0x00
HdMap Capacity = 0x04 0x05 0x04 0x03 0x09 0x09 0x00 0x00