Format version = 0x0002
Версия controller firmware = 58.A9D
Версия servo firmware = 01.0L
Версия overley firmware = 58.A9D
Версия surface format = A1.000
Версия read channel firmware = 06.12Q85
Количество пластин = 2
Количество физических головок = 3
Количество используемых головок = 3
Карта используемых головок =  0 1 2
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 240
Количество треков в SA = 128
Обороты двигателя = 7230
Количество треков в UA = 0
Cylinder skew = 25
Head skew = 77
Cluster Skew = 130
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 8Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x42B1
MicroP Vendor = 0x0000
MicroP Rev = 0x42B1
Channel Chip Vendor = 0x00E6
Channel chip Rev = 0x0011
Preamp Vendor = 0x0001
Preamp Rev = 0x0001
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC коррекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 168Gb
Drive Format Type = 0
 
Код производителя пластин - K
Код производителя головок - 7
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0003
used_heads = 0x0003
cur_capacity = 0x09D0
max_fmt_LBAs = 490825440 - 251Gb
target_capacity = 0x0001
max_target_LBAs = 490234751 - 251Gb
hq_capacity = 0x0001
max_HQ_LBAs = 490825440 - 251Gb
final_capacity = 0x0001
z0_dtpi = 0x0001D97A
z0_kfci = 0x00000001
cur_svo_TPI = 0x00023668
cur_data_TPI_0 = 0x00023668
cur_data_TPI_1 = 0x00023668
cur_data_TPI_2 = 0x00021301
cur_data_TPI_3 = 0x00000000
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x035A
cur_KFCI_1 = 0x0306
cur_KFCI_2 = 0x0370
cur_KFCI_3 = 0x0000
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 167626368 - 85Gb
max_LBA_for_head_1 = 151181856 - 77Gb
max_LBA_for_head_2 = 172017216 - 88Gb
max_LBA_for_head_3 = 0 - 0Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x000232F9
max_user_cyls_for_head_1 = 0x000232F9
max_user_cyls_for_head_2 = 0x00020FD2
max_user_cyls_for_head_3 = 0x00000000
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x00023700
max_virt_cyls_for_head_1 = 0x00023700
max_virt_cyls_for_head_2 = 0x00021390
max_virt_cyls_for_head_3 = 0x00000000
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0100
rsvd_data_cyls = 0x0080
max_user_svo_cyls = 0x00023278
max_svo_cyls = 0x00023700
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0080
trks_per_clstr_for_head_0 = 0x0080
trks_per_clstr_for_head_1 = 0x0080
trks_per_clstr_for_head_2 = 0x0078
trks_per_clstr_for_head_3 = 0x0000
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x01 0x01 0x03 0x00 0x00 0x00 0x00 0x00
HdMap Capacity = 0x03 0x07 0x02 0x00 0x00 0x00 0x00 0x00