Format version = 0x0002
Версия controller firmware = 58.7RD
Версия servo firmware = 01.0F
Версия overley firmware = 58.7RD
Версия surface format = EX.042
Версия read channel firmware = 06.12Q79
Количество пластин = 3
Количество физических головок = 6
Количество используемых головок = 4
Карта используемых головок =  0 1 2 3 4 5
Тип накопителя = Desktop 3.5 Inch
Количество зон = 21
Количество servo wedges = 240
Количество треков в SA = 128
Обороты двигателя = 7230
Количество треков в UA = 0
Cylinder skew = 25
Head skew = 77
Cluster Skew = 130
Code Residence = 6
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 16Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x42B1
MicroP Vendor = 0x0000
MicroP Rev = 0x42B1
Channel Chip Vendor = 0x00E6
Channel chip Rev = 0x0011
Preamp Vendor = 0x0000
Preamp Rev = 0x0002
Power IC vendor = 0x0000
Power IC Rev = 0x0000
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 1
Number of bytes corrected by OTF = 22
Number of bytes corrected by FW burst corr = 43
No. of ecc bytes in read/write long sector = 55
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 160Gb
Drive Format Type = 1
 
Код производителя пластин - K
Код производителя головок - 7
 
Конфигурация накопителя
Format version = 0x0101
DCM Selection = 0x0001
cur_stroke = 0x0001
phy_heads = 0x0006
used_heads = 00004
cur_capacity = 0x0C80
max_fmt_LBAs = 625177728 - 320Gb
target_capacity = 0x0002
max_target_LBAs = 625142447 - 320Gb
hq_capacity = 0x0002
max_HQ_LBAs = 625821840 - 320Gb
final_capacity = 0x0002
z0_dtpi = 0x0001D97A
z0_kfci = 0x00000002
cur_svo_TPI = 0x00023668
cur_data_TPI_0 = 0x00023668
cur_data_TPI_1 = 0x000224B4
cur_data_TPI_2 = 0x00021301
cur_data_TPI_3 = 0x000224B4
cur_data_TPI_4 = 0x00000000
cur_data_TPI_5 = 0x00000000
cur_data_TPI_6 = 0x00000000
cur_data_TPI_7 = 0x00000000
cur_data_TPI_8 = 0x00000000
cur_data_TPI_9 = 0x00000000
cur_KFCI_0 = 0x0320
cur_KFCI_1 = 0x0320
cur_KFCI_2 = 0x0320
cur_KFCI_3 = 0x0320
cur_KFCI_4 = 0x0000
cur_KFCI_5 = 0x0000
cur_KFCI_6 = 0x0000
cur_KFCI_7 = 0x0000
cur_KFCI_8 = 0x0000
cur_KFCI_9 = 0x0000
max_LBA_for_head_0 = 156294432 - 80Gb
max_LBA_for_head_1 = 156294432 - 80Gb
max_LBA_for_head_2 = 156294432 - 80Gb
max_LBA_for_head_3 = 156294432 - 80Gb
max_LBA_for_head_4 = 0 - 0Gb
max_LBA_for_head_5 = 0 - 0Gb
max_LBA_for_head_6 = 0 - 0Gb
max_LBA_for_head_7 = 0 - 0Gb
max_LBA_for_head_8 = 0 - 0Gb
max_LBA_for_head_9 = 0 - 0Gb
max_user_cyls_for_head_0 = 0x00023406
max_user_cyls_for_head_1 = 0x0002226A
max_user_cyls_for_head_2 = 0x000210CE
max_user_cyls_for_head_3 = 0x0002226A
max_user_cyls_for_head_4 = 0x00000000
max_user_cyls_for_head_5 = 0x00000000
max_user_cyls_for_head_6 = 0x00000000
max_user_cyls_for_head_7 = 0x00000000
max_user_cyls_for_head_8 = 0x00000000
max_user_cyls_for_head_9 = 0x00000000
max_virt_cyls_for_head_0 = 0x00023700
max_virt_cyls_for_head_1 = 0x00022548
max_virt_cyls_for_head_2 = 0x00021390
max_virt_cyls_for_head_3 = 0x00022548
max_virt_cyls_for_head_4 = 0x00000000
max_virt_cyls_for_head_5 = 0x00000000
max_virt_cyls_for_head_6 = 0x00000000
max_virt_cyls_for_head_7 = 0x00000000
max_virt_cyls_for_head_8 = 0x00000000
max_virt_cyls_for_head_9 = 0x00000000
rsvd_svo_cyls = 0x0100
rsvd_data_cyls = 0x0080
max_user_svo_cyls = 0x00023385
max_svo_cyls = 0x00023700
trks_per_clstr_svo = 0x0080
trks_per_clstr_rsvd = 0x0080
trks_per_clstr_for_head_0 = 0x0080
trks_per_clstr_for_head_1 = 0x007C
trks_per_clstr_for_head_2 = 0x0078
trks_per_clstr_for_head_3 = 0x007C
trks_per_clstr_for_head_4 = 0x0000
trks_per_clstr_for_head_5 = 0x0000
trks_per_clstr_for_head_6 = 0x0000
trks_per_clstr_for_head_7 = 0x0000
trks_per_clstr_for_head_8 = 0x0000
trks_per_clstr_for_head_9 = 0x0000
HdMap TPI = 0x01 0x02 0x03 0x02 0x00 0x00 0x00 0x00
HdMap Capacity = 0x0B 0x0B 0x0B 0x0B 0x00 0x00 0x00 0x00