Format version = 0x0002
Версия controller firmware = 06.2EA
Версия servo firmware = 02.0E
Версия overley firmware = 06.2EA
Версия surface format = A1.013
Версия read channel firmware = A1.29110
Количество пластин = 2
Количество физических головок = 4
Количество используемых головок = 4
Карта используемых головок = 0 1 2 3
Тип накопителя = Mobile 2.5 Inch
Количество зон = 21
Количество servo wedges = 248
Количество треков в SA = 256
Обороты двигателя = 5400
Количество треков в UA = 0
Cylinder skew = 33
Head skew = 78
Cluster Skew = 112
Code Residence = 5
Тип PCBA = Entek
Тип интерфейса = Serial ATA
Установленная память = 32Mb
 
Информация о комплектующих
Controller chip Vendor = 0x0000
Controller chip rev = 0x7412
MicroP Vendor = 0x0000
MicroP Rev = 0x7412
Channel Chip Vendor = 0x0039
Channel chip Rev = 0x0023
Preamp Vendor = 0x0001
Preamp Rev = 0x0003
Power IC vendor = 0x0000
Power IC Rev = 0x001C
 
Информация о ECC корекции
No. of interleaves in OTF ECC corr = 4
Number of bytes corrected by OTF = 26
Number of bytes corrected by FW burst corr = 185
No. of ecc bytes in read/write long sector = 245
 
Информация о формате
Tracks per inch (in KTPI) = 0
Area density = 375Gb
Drive Format Type = 0