Identify Drive Data:
General config. bit info:                   0C5A	(Word 0)
Logical Cyls:                               3FFF	(Word 1)
Reserved(removable cyls.):                  C837	(Word 2)
Logical Hds:                                0010	(Word 3)
V.S.(Bytes/trk):                            0000	(Word 4)
V.S.(Bytes/sect):                           0000	(Word 5)
Logical Sects. per track:                   003F	(Word 6)
V.S.(Sect Gap Bytes):                       0000	(Word 7)
V.S.(Sync Field Bytes):                     0000	(Word 8)
V.S.(Zilch):                                0000	(Word 9)
Serial Number:                                          9QM3EXAX	(Word 10-19)
V.S.(Controller type):                      0000	(Word 20)
V.S.(Controller Buf. Size):                 4000	(Word 21)
V.S.(# of ECC Bytes):                       0004	(Word 22)
Firmware Rev:                               SD81    	(Word 23-26)
Model:                                      ST3500820AS                             	(Word 27-46)
Max. Supported Mult. Size:                  8010	(Word 47)
Reserved(Double word capable):              0000	(Word 48)
Capabilities:                               2F00	(Word 49)
Reserved:                                   4000	(Word 50)
PIO xfer cycle timing mode:                 0200	(Word 51)
DMA xfer cycle timing mode:                 0200	(Word 52)
Words 54-58, 64-70 are valid:               0007	(Word 53)
Num. of current Log. Cyls:                  3FFF	(Word 54)
Num. of current Log. Hds:                   0010	(Word 55)
Num. of current Log. Sects:                 003F	(Word 56)
Current User Capacity:                      00FBFC10  16514064	(Word 57-58)
Current Multiple Size:                      0010	(Word 59)
Total User Capacity:                        0FFFFFFF  268435455	(Word 60-61)
V.S.(Single word DMA):                      0000	(Word 62)
DMA mode set/DMA modes supported:           0407	(Word 63)
Advanced PIO Modes:                         0003	(Word 64)
Multi DMA Xfer time:                        0078	(Word 65)
Recomended multi DMA time:                  0078	(Word 66)
Min. Pio time w/o flow cntrl:               0078	(Word 67)
Min. Pio time with IORDY flow:              0078	(Word 68)
Reserved:                                   0000	(Word 69)
Reserved:                                   0000	(Word 70)
Reserved:                                   0000	(Word 71)
Reserved:                                   0000	(Word 72)
Reserved:                                   0000	(Word 73)
Reserved:                                   0000	(Word 74)
Queue Depth:                                001F	(Word 75)
Reserved:                                   0506	(Word 76)
Reserved:                                   0000	(Word 77)
Reserved:                                   0040	(Word 78)
Reserved:                                   0040	(Word 79)
Major Version Number:                       01F0	(Word 80)
Minor Version Number:                       0029	(Word 81)
Command Set Supported:                      346B	(Word 82)
Command Set Supported:                      7D01	(Word 83)
Command Set/Feature Supported:              4123	(Word 84)
Command Set/Feature Enabled:                3469	(Word 85)
Command Set/Feature Enabled:                BC01	(Word 86)
Command Set/Feature Default:                4123	(Word 87)
UDMA Mode Set/UDMA modes supported:         007F	(Word 88)
Security Erase Time:                        0034	(Word 89)
Enhanced Security Erase Time:               0034	(Word 90)
Security Status:                            0021	(Word 128)
HDA Capacity:                               3A386030  976773168	(Word 129-130)
Native Capacity:                            3A386030  976773168	(Word 131-132)
Incremental Code Version:                   0000	(Word 133)
Compaq Word:                                0002	(Word 134)
Inter-Sector Time:                          0140	(Word 135)
ATA Pad Control:                            0100	(Word 136)
uSecs. Delay for Disk Commands:             5000	(Word 137)
Write Queue Algorithm Selection:            3C06	(Word 138)
Write Queuing Enabled:                      3C0A	(Word 139)
Write Caching Enabled on pwr up:            0000	(Word 140)
F.W. Seq Wrt det. On/Auto-Seq Wrts On:      003C	(Word 141)
# of Rd Segs/Rd Look-ahead on @ Pwr.up:     0000	(Word 142)
Auto-Sequential Reads Enabled:              0008	(Word 143)
Offline scan time/offline scan cnt.:        0000	(Word 144)
Write Sparing Enabled:                      0000	(Word 145)
Read Sparing Enabled:                       000F	(Word 146)
Offline seek period/Offline Timer:          0280	(Word 147)
SMART seek err adj/Iffy Marks disable:      0000	(Word 148)
Download Flash Size:                        0000	(Word 149)
Rd Buffer size:                             0008	(Word 150)
Offline sparing enabled:                    0000	(Word 151)
Wrt Q Entry discarding Enabled:             0000	(Word 152)
IRQ regen. delay/Auto Seq wrt IRQ delay:    0000	(Word 153)
V.S.:                                       0000	(Word 154)
V.S.:                                       0000	(Word 155)
V.S.:                                       0000	(Word 156)
V.S.:                                       0000	(Word 157)
Drive Type:                                 2700	(Word 158)
AT Stuff Format Ver:                        8000	(Word 159)
