TetonST 2.0 SATA Moose Gen 3.0 (RAP fmt 10 ) w/sdff (RV )
Product FamilyId: 27, MemberId: 04
HDA SN: 9QM2EG5Q, RPM: 7206, Wedges: 108, Heads: 4, Lbas: 3A386030, PreampType:
45 09
PCBA SN: 0000C8366W2V, Controller: TETONST_2(639D)(3-0E-3-5), Channel: AGERE_COPPERHEAD_LITE, PowerAsic: MCKINLEY Rev 04, BufferBytes: 2000000
Package Version: MS0100.MXD1.AD090B.MX15    , Package P/N: 100504103, Package Builder ID: 3K,
Package Build Date: 01/16/2008, Package Build Time: 16:28:26, Package CFW Version: MS01.MXD1.00052452.3K00,
Package SFW1 Version: B000, Package SFW2 Version: C0FE, Package SFW3 Version: C0FA, Package SFW4 Version: ----
Controller FW Rev: 01161628, CustomerRel: MX15, Changelist: 00052452, ProdType:
MS01.MXD1, Date: 01/16/2008, Time: 162826, UserId: 00000761
Servo FW Rev: C0FE
RAP Format Rev: 0092, Contents Rev: 15 05 10 06
Features:
- Quadradic Equation AFH enabled
- VBAR with adjustable zone boundaries enabled
- Volume Based Sparing enabled
- IOEDC enabled
- IOECC enabled
- DERP Read Retries enabled    