

Test  : Data buffers reading (terminal)
Starting block........... : 0x0
Amount................... : 0xFF
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\RAMDump\Data Buff 0x00000000 (0x000000FF).dmp
Result.................................. : Error

Buffers reading terminated by user

COM transfer baud rate setted to 921000


Test  : Data buffers reading (terminal)
Starting block........... : 0x0
Amount................... : 0xFF
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\RAMDump\Data Buff 0x00000000 (0x000000FF).dmp
Result.................................. : Ok



Test  : RAM reading (by terminal)
Starting address......... : 0x0
Amount................... : 0xFFF
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\RAMDump\RAM 0x00000000 (0x00000FFF).dmp
Result.................................. : Ok


Terminal : Detecting SA bounds...
Trying to load CERT
Result.................................. : Ok
Detection SA bounds by MUX
SA bounds defined

Terminal : Detecting SA bounds...
Trying to load CERT
Result.................................. : Ok
Detection SA bounds by MUX
SA bounds defined


Test  : Reading SA surface by PCHS (terminal)
Location (PCHS).......... : 0xE98E : 0x0 : 0x0
Amount................... : 0x0
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\PCHSDump\PCHS 0x00E98E_0x00_0x0000(0x0000).chs
Result.................................. : Ok


Terminal : Detecting SA bounds...
Trying to load CERT
Result.................................. : Ok
Detection SA bounds by MUX
SA bounds defined


Test  : Reading SA surface by PCHS (terminal)
Location (PCHS).......... : 0xE98E : 0x0 : 0x0
Amount................... : 0x280
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\PCHSDump\PCHS 0x00E98E_0x00_0x0000(0x0280).chs
Surface reading error (0xE98E : 0x0 : 0x0)
HDD reply :

    Code - 47  Track 0E98E.0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 47 -> Missed data sync byte

Surface reading error (0xE98E : 0x0 : 0x0)
HDD reply :

    Code - 43  Track 0E98E.0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 43 -> Data ECC error

Surface reading error (0xE98E : 0x0 : 0x0)
HDD reply :

    Code - 47  Track 0E98E.0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 47 -> Missed data sync byte

Surface reading error (0xE98E : 0x0 : 0x1)
HDD reply :

    Code - 47  Track 0E98E.0.001  Sns 001  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 47 -> Missed data sync byte

Surface reading error (0xE98E : 0x0 : 0x1)
HDD reply :

    Code - 43  Track 0E98E.0.001  Sns 001  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 43 -> Data ECC error

Surface reading error (0xE98E : 0x0 : 0x2)
HDD reply :

    Code - 47  Track 0E98E.0.002  Sns 002  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 47 -> Missed data sync byte

Result.................................. : Error


Surface reading error (0xE98E : 0x0 : 0x2)
HDD reply :

    Code - 43  Track 0E98E.0.002  Sns 002  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 43 -> Data ECC error


Terminal : Detecting SA bounds...
Trying to load CERT
Result.................................. : Ok
Detection SA bounds by MUX
SA bounds defined


Test  : Reading SA surface by PCHS (terminal)
Location (PCHS).......... : 0xE98F : 0x0 : 0x0
Amount................... : 0x280
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\PCHSDump\PCHS 0x00E98F_0x00_0x0000(0x0280).chs
Surface reading error (0xE98F : 0x0 : 0x0)
HDD reply :

    Code - 43  Track 0E98F.0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 43 -> Data ECC error

Surface reading error (0xE98F : 0x0 : 0x0)
HDD reply :

    Code - 43  Track 0E98F.0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 43 -> Data ECC error

Result.................................. : Error


Surface reading error (0xE98F : 0x0 : 0x0)
HDD reply :

    Code - 43  Track 0E98F.0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 0269A988

Description............................. : Err 43 -> Data ECC error


Executing user command.................. : Switch HDD to ATA mode (Age=50)

Executing user command.................. : Load CERT

Executing user command.................. : Show zones distribution

Executing user command.................. : Show Alt list (remap)

Executing user command.................. : Show User track slip list (P-List)

Executing user command.................. : Show Reserved track slip list

Executing user command.................. : Show buffers map

Executing user command.................. : Show ROM information

Executing user command.................. : Show PCB information

COM transfer baud rate setted to 9600

Executing user command.................. : Show ROM information

COM transfer baud rate setted to 921000


Test  : ROM reading (terminal)
ROM file type............ : Programmator image
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\ROM\ROM.bin
Result.................................. : Ok


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading SA surface by PCHS (terminal)
Location (PCHS).......... : 0xE31B : 0x0 : 0x0
Amount................... : 0x180
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Barracuda 7200.7\ST340014AS-3.00-4MQ06QRX\Data\PCHSDump\PCHS 0x00E31B_0x00_0x0000(0x0180).chs
Result.................................. : Ok


COM transfer baud rate setted to 9600

Executing user command.................. : Switch HDD to ATA mode (Age=50)
