Identify Drive Data:
General config. bit info:                   0C5A
Logical Cyls:                               3FFF
Reserved(removable cyls.):                  0000
Logical Hds:                                0010
V.S.(Bytes/trk):                            0000
V.S.(Bytes/sect):                           0000
Logical Sects. per track:                   003F
V.S.(Sect Gap Bytes):                       0000
V.S.(Sync Field Bytes):                     0000
V.S.(Zilch):                                0000
Serial Number:                              7BQ0QGAJ            
V.S.(Controller type):                      0000
V.S.(Controller Buf. Size):                 0400
V.S.(# of ECC Bytes):                       0000
Firmware Rev:                               3.09    
Model:                                      ST310232A                               
Max. Supported Mult. Size:                  8010
Reserved(Double word capable):              0000
Capabilities:                               2F00
Reserved:                                   0000
PIO xfer cycle timing mode:                 0200
DMA xfer cycle timing mode:                 0200
Words 54-58, 64-70 are valid:               0007
Num. of current Log. Cyls:                  3FFF
Num. of current Log. Hds:                   0010
Num. of current Log. Sects:                 003F
Current User Capacity:                      00FBFC10  16514064
Current Multiple Size:                      0010
Total User Capacity:                        01314312  20005650
V.S.(Single word DMA):                      0000
DMA mode set/DMA modes supported:           0407
Advanced PIO Modes:                         0003
Multi DMA Xfer time:                        0078
Recomended multi DMA time:                  0078
Min. Pio time w/o flow cntrl:               00F0
Min. Pio time with IORDY flow:              0078
Reserved:                                   0000
Reserved:                                   0000
Reserved:                                   0000
Reserved:                                   0000
Reserved:                                   0000
Reserved:                                   0000
Queue Depth:                                0000
Reserved:                                   0000
Reserved:                                   0000
Reserved:                                   0000
Reserved:                                   0000
Major Version Number:                       001E
Minor Version Number:                       0000
Command Set Supported:                      3069
Command Set Supported:                      4001
Command Set/Feature Supported:              4000
Command Set/Feature Enabled:                3069
Command Set/Feature Enabled:                0001
Command Set/Feature Default:                4000
UDMA Mode Set/UDMA modes supported:         001F
Security Erase Time:                        0000
Enhanced Security Erase Time:               0000
Security Status:                            0000
HDA Capacity:                               01843608  25441800
Native Capacity:                            01843608  25441800
Incremental Code Version:                   2020
Compaq Word:                                0002
Inter-Sector Time:                          0000
ATA Pad Control:                            C001
uSecs. Delay for Disk Commands:             0000
Write Queue Algorithm Selection:            0002
Write Queuing Enabled:                      0401
Write Caching Enabled on pwr up:            0801
F.W. Seq Wrt det. On/Auto-Seq Wrts On:      0140
# of Rd Segs/Rd Look-ahead on @ Pwr.up:     0401
Auto-Sequential Reads Enabled:              0000
Offline scan time/offline scan cnt.:        3C24
Write Sparing Enabled:                      0201
Read Sparing Enabled:                       4001
Offline seek period/Offline Timer:          3CB4
SMART seek err adj/Iffy Marks disable:      0100
Download Flash Size:                        0100
Rd Buffer size:                             0072
Offline sparing enabled:                    3001
Wrt Q Entry discarding Enabled:             0001
IRQ regen. delay/Auto Seq wrt IRQ delay:    0140
V.S.:                                       0000
V.S.:                                       0000
V.S.:                                       FFFF
V.S.:                                       094B
Drive Type:                                 0005
AT Stuff Format Ver:                        0009
