Error switching COM port data transfer baud rate
Error switching COM port data transfer baud rate
Terminal : error detecting HDD terminal baud rate


Test  : RAM reading (by terminal)
Starting address......... : 0x0
Amount................... : 0xFFF
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\RAMDump\RAM 0x00000000 (0x00000FFF).dmp
Result.................................. : Ok


COM transfer baud rate setted to 921000


Test  : Data buffers reading (terminal)
Starting block........... : 0x0
Amount................... : 0xFFF
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\RAMDump\Data Buff 0x00000000 (0x00000FFF).dmp
Result.................................. : Ok


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading SA surface by PCHS (terminal)
Location (PCHS).......... : 0xCC46 : 0x0 : 0x0
Amount................... : 0x201
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\PCHS 0x00CC46_0x00_0x0000(0x0201).chs
Surface reading error (0xCC46 : 0x0 : 0x200)
HDD reply :

    Code - FE  Track FFFFF(0CC46).0.200  Sns 200  Rty F7FF.FF.80FF  Rtf 1800  LBA 03919766

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC46 : 0x0 : 0x200)
HDD reply :

    Code - FE  Track FFFFF(0CC46).0.200  Sns 200  Rty F7FF.FF.80FF  Rtf 1800  LBA 03919766

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC46 : 0x0 : 0x200)
HDD reply :

    Code - FE  Track FFFFF(0CC46).0.200  Sns 200  Rty F7FF.FF.80FF  Rtf 1800  LBA 03919766

Description............................. : Err FE -> Invalid address passed to Niwot

Result.................................. : Error



Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC48
Stopping cylinder........ : 0xCC48
Head..................... : 0x0
SPT...................... : 0x201
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCC48 : 0x0 : 0x200)
HDD reply :

    Code - FE  Track FFFFF(0CC48).0.200  Sns 200  Rty F7FF.FF.80FF  Rtf 1800  LBA 03919766

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC48 : 0x0 : 0x200)
HDD reply :

    Code - FE  Track FFFFF(0CC48).0.200  Sns 200  Rty F7FF.FF.80FF  Rtf 1800  LBA 03919766

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC48 : 0x0 : 0x200)
HDD reply :

    Code - FE  Track FFFFF(0CC48).0.200  Sns 200  Rty F7FF.FF.80FF  Rtf 1800  LBA 03919766

Description............................. : Err FE -> Invalid address passed to Niwot

Reading track 0xCC48.................... : Error

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC48
Stopping cylinder........ : 0xCC48
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC48.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC4A
Stopping cylinder........ : 0xCC4A
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC4A.................... : Ok
Terminal : error detecting HDD terminal baud rate

COM transfer baud rate setted to 9600


Test  : ROM reading (terminal)
ROM file type............ : Programmator image
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\ROM\ROM.bin
Result.................................. : Ok


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined

COM transfer baud rate setted to 921000

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCD9
Stopping cylinder........ : 0xCCF7
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Terminal : reply timeout error
Terminal : reply timeout error
Terminal : reply timeout error
Terminal : reply timeout error
Terminal : reply timeout error
Terminal : reply timeout error
Surface reading error (0xCCD9 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading terminated by user

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCD9
Stopping cylinder........ : 0xCCF7
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCCD9 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xA)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xA)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xB)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xB)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xC)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xC)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xD)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xD)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xE)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xE)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xF)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0xF)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x10)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x10)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x10)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x11)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x11)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x12)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x12)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x13)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCD9 : 0x0 : 0x13)
HDD reply :

    Code - FE  Track 0CCD9.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCDA
Stopping cylinder........ : 0xCCDA
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCCDA.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCDB
Stopping cylinder........ : 0xCCE7
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCCDB : 0x0 : 0x0)
HDD reply :

    Code - FE  Track 0CCDB.0.100  Sns 100

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x0)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x0)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x1)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x1)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x2)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x2)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x3)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x3)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x4)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x4)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x5)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x5)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x6)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x6)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCCDB : 0x0 : 0x7)
HDD reply :

    Code - FE  Track 0CCDB.0.000  Sns 000

Description............................. : Err FE -> Invalid address passed to Niwot


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCDC
Stopping cylinder........ : 0xCCDC
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCCDC.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCF4
Stopping cylinder........ : 0xCCF4
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCCF4.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCCF6
Stopping cylinder........ : 0xCCF6
Head..................... : 0x0
SPT...................... : 0x1F2
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCCF6.................... : Ok

COM transfer baud rate setted to 9600

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC02
Stopping cylinder........ : 0xCC02
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCC02 : 0x0 : 0x0)
HDD reply :

    Code - 47  Track FFFFF(0CC02).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err 47 -> Missed data sync byte

Surface reading error (0xCC02 : 0x0 : 0x0)
HDD reply :

    Code - 43  Track FFFFF(0CC02).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err 43 -> Data ECC error

Surface reading error (0xCC02 : 0x0 : 0x0)
HDD reply :

    Code - 43  Track FFFFF(0CC02).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err 43 -> Data ECC error


COM transfer baud rate setted to 921000

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC0C
Stopping cylinder........ : 0xCC0C
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCC0C : 0x0 : 0x0)
HDD reply :

    Code - 47  Track FFFFF(0CC0C).0.004  Sns 004  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err 47 -> Missed data sync byte

Buffers reading terminated by user

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC18
Stopping cylinder........ : 0xCC18
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC18.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC1A
Stopping cylinder........ : 0xCC1A
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC1A.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC26
Stopping cylinder........ : 0xCC26
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCC26 : 0x0 : 0x0)
HDD reply :

    Code - 47  Track FFFFF(0CC26).0.004  Sns 004  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err 47 -> Missed data sync byte

Buffers reading terminated by user

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC32
Stopping cylinder........ : 0xCC32
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC32.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC34
Stopping cylinder........ : 0xCC34
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC34.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC36
Stopping cylinder........ : 0xCC36
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC36.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC38
Stopping cylinder........ : 0xCC38
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC38.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC40
Stopping cylinder........ : 0xCC40
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC40.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC5E
Stopping cylinder........ : 0xCC5E
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC5E.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC66
Stopping cylinder........ : 0xCC66
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC66.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC67
Stopping cylinder........ : 0xCC67
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Surface reading error (0xCC67 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC67 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC67).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading terminated by user

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC68
Stopping cylinder........ : 0xCC68
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Buffers reading terminated by user

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC68
Stopping cylinder........ : 0xCC69
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC68.................... : Ok
Surface reading error (0xCC69 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC69 : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CC69).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC6A
Stopping cylinder........ : 0xCC6D
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC6A.................... : Ok
Surface reading error (0xCC6B : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x18)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x18)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x19)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x19)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x1F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x21)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x21)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x22)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x22)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x23)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x23)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x24)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x24)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x25)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x25)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x26)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x26)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x27)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x27)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x28)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x28)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x29)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x29)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x2F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x30)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x30)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x30)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x31)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x31)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x32)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x32)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x33)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x33)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x34)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x34)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x35)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x35)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x36)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x36)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x37)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x37)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x38)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x38)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x39)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x39)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x3F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x40)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x40)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x40)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x41)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x41)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x42)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x42)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x43)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x43)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x44)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x44)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x45)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x45)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x46)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x46)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x47)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x47)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x48)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x48)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x49)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x49)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x4F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x50)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x50)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x50)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x51)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x51)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x52)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x52)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x53)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x53)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x54)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x54)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x55)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x55)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x56)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x56)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x57)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x57)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x58)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x58)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x59)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x59)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x5F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x60)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x60)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x60)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x61)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x61)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x62)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x62)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x63)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x63)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x64)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x64)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x65)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x65)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x66)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x66)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x67)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x67)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x68)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x68)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x69)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x69)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x6F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x70)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x70)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x70)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x71)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x71)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x72)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x72)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x73)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x73)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x74)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x74)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x75)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x75)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x76)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x76)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x77)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x77)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x78)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x78)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x79)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x79)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x7F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x80)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x80)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x80)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x81)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x81)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x82)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x82)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x83)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x83)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x84)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x84)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x85)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x85)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x86)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x86)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x87)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x87)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x88)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x88)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x89)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x89)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x8F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x90)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x90)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x90)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x91)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x91)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x92)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x92)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x93)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x93)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x94)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x94)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x95)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x95)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x96)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x96)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x97)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x97)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x98)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x98)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x99)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x99)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x9F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xA9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xAF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xB9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xBF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xC9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xCF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xD9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xDF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xE9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xED)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xED)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xEF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF0)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF1)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF2)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF3)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF4)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF5)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF6)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF7)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF8)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xF9)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFA)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFB)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFC)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFD)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFE)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0xFF)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x100)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x100)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x100)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x101)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x101)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x102)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x102)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x103)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x103)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x104)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x104)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x105)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x105)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x106)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x106)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x107)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x107)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x108)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x108)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x109)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x109)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10A)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10B)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10C)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10D)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10E)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x10F)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x110)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x110)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x110)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x111)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x111)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x112)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x112)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x113)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x113)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x114)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x114)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x115)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x115)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x116)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC6B : 0x0 : 0x116)
HDD reply :

    Code - FE  Track FFFFF(0CC6B).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC6E
Stopping cylinder........ : 0xCC6E
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC6E.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC7A
Stopping cylinder........ : 0xCC7A
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC7A.................... : Ok

Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCC9E
Stopping cylinder........ : 0xCC9F
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCC9E.................... : Ok
Surface reading error (0xCC9F : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x18)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x18)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x19)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x19)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1A)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1A)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1B)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1B)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1C)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1C)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1D)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1D)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1E)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1E)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1F)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x1F)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x21)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x21)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x22)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x22)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x23)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x23)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x24)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x24)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x25)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x25)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x26)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x26)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x27)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x27)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x28)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x28)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x29)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x29)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2A)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2A)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2B)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2B)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2C)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2C)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2D)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2D)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2E)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2E)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCC9F : 0x0 : 0x2F)
HDD reply :

    Code - FE  Track FFFFF(0CC9F).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCD12
Stopping cylinder........ : 0xCD1F
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCD12.................... : Ok
Surface reading error (0xCD13 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD13 : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CD13).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot


Terminal : Detecting SA bounds...
Detection SA bounds by MUX
SA bounds defined


Test  : Reading tracks group by PCHS (terminal)
Starting cylinder........ : 0xCD2C
Stopping cylinder........ : 0xCD2D
Head..................... : 0x0
SPT...................... : 0x1FF
HDD profile forlder...... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\Momentus\ST9808211A-3.00-3LG0VKF7\Data\PCHSDump\

Reading track 0xCD2C.................... : Ok
Surface reading error (0xCD2D : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x0)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x2)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x3)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x4)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x5)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x6)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x7)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x8)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x9)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xA)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xB)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xC)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xD)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xE)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0xF)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x10)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x11)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x12)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x13)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x14)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x15)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x16)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x17)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x18)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x18)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x19)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x19)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1A)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1A)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1B)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1B)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1C)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1C)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1D)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1D)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1E)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1E)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1F)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x1F)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x20)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x21)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x21)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x22)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x22)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x23)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x23)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x24)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x24)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x25)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x25)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x26)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot

Surface reading error (0xCD2D : 0x0 : 0x26)
HDD reply :

    Code - FE  Track FFFFF(0CD2D).0.000  Sns 000  Rty F7FF.FF.80FF  Rtf 1800  LBA 051B470E

Description............................. : Err FE -> Invalid address passed to Niwot


Executing user command.................. : Load CERT

Executing user command.................. : Show zones distribution

Executing user command.................. : Show Alt list (remap)

Executing user command.................. : Show User track slip list (P-List)

Executing user command.................. : Show Reserved track slip list

Executing user command.................. : Show buffers map

Executing user command.................. : Show ROM information

COM transfer baud rate setted to 9600

Executing user command.................. : Show ROM information

Executing user command.................. : Show PCB information
Error switching COM port data transfer baud rate
