Interface task reset1024k x 16 buffer detected 
SNOWMASS - 1_Disk    3.75  11-20-01 13:27 

                          Power Cycling
ATReset
Head Mask 0002 - Switch to full int.
              Spin Ready

Sweeping 189 Cyls
PMaster
(
T>SNOWMASS - 1_Disk    3.75  11-20-01 13:27 
Built for SNOWMASS,SaratogaII,NAPA,TI1761 PreAmp,VTC5833 PreAmp,InternalSpin,SVC125,OneToOne,2Disk,LowDelta,196 Servos,7200RPM,8Pole,NonModGray,90MHz,Code DRAM,Early Exit,RwFeat=0000
(
T>/2
2>x
Command Inactive - No VALID Cert Code Detected
2>((VALID Cert Disk Code Detected - Revision # 3.75

2>x
 Zone 0:  0015 - 17AF   833   552.156
 Zone 1:  17B0 - 2FE0   833   552.156
 Zone 2:  2FE1 - 40F0   833   552.156
 Zone 3:  40F1 - 5700   784   510.588
 Zone 4:  5701 - 696B   784   510.588
 Zone 5:  696C - 7D00   718   477.647
 Zone 6:  7D01 - 8B8B   686   454.117
 Zone 7:  8B8C - 9B24   653   435.294
 Zone 8:  9B25 - A9D6   616   414.117
 Zone 9:  A9D7 - BA00   588   385.882
 Zone A:  BA01 - C4BA   548   371.092
 Zone B:  C4BB - D105   522   352.941
 Zone C:  D106 - DC91   490   330.756
Sys= 7000-7028   02B9 SPTK on sys trks 
Total LBAs = 0263190A

