Interface task reset512k x 32 SDRAM
TONKA15 - 1_Disk    S.68   03-14-06 11:24

Buzz  - Head Mask FFFF - Switch to full int.
              Spin Ready
(P)PATA Reset
Failed sys sect. write

Read Ver Retrys

Read Ver Retrys

Read Ver Retrys

Read Ver Retrys

Read Ver Failure!
Failed sys sect. write
Unable To Load Overlay 01|000A
(
T>Eng Rev = .0F0
TONKA15 - 2_Disk    3.AAH  03-14-06 11:27 AAH,35_P_5_S0,4T 
CERT Rev = .0C2
NONE
Mask Rom Rev = S.68  
Unique Descriptor = .5S0
(
T>TONKA15 - 2_Disk    3.AAH  03-14-06 11:27 AAH,35_P_5_S0,4T 
Built for TONKA15,PITKIN,Redback,TI1810 PreAmp,Agere7531 PreAmp,InternalSpin,McKinleyDT,OneToOne,3Disk,LowDelta,220 Servos,7200RPM,8Pole,NonModGray,133MHz,Code DRAM,Early Exit,Stall Converter,RwFeat=0002,SeaDex,VBAR,MDW
(
T>((VALID Cert Disk Code Detected - Revision # .0C2

T>k
Head Mask = FF
 Map 00 to 00 00
 Map 01 to 01 01
 Map 02 to 02 02
 Map 03 to 03 03
 Map 04 to 04 04
 Map 05 to 05 05
T>Pgm=00 Trk=FFFFF(15FEB:00[1722A]).3(3).004(FFF) Zn=0 Err=00 ErCt=0000 Hlth=0000 CHlth=0000 Ready LBA=000013B4
Age=50 Type=15 MxCyl=1DC87 MxHd=3 MxSct=000 BSz=002M TCode=00FF0201 ThermFlts=0000
(
T>y
                  PhysCyl   GrayCyl 
 1st Sys Cyl      00015EEF  00016FBD 
 1st 0 Offset Cyl 00015EF9  00016FC7 
 1st App Code Cyl 00015F05  00016FD3 
 2nd App Code Cyl 00015F07  00016FD5 
 2nd 0 Offset Cyl 00015F13  00016FE1 
 3rd App Code Cyl 00015F1F  00016FED 
 4th App Code Cyl 00015F21  00016FEF 
 1st Adaptive Cyl 00015F23  00016FF1 
 1st UsrDfect Cyl 00015F25  00016FF3 
 1st Alt Pool Cyl 00015F2D  00016FFB 
 2nd UsrDfect Cyl 00015F4B  00017019 
 1st CertCode Cyl 00015F53  00017021 
 1st IntfCode Cyl 00015F57  00017025 
 1st Intf Sys Cyl 00015F5B  00017029 
 1st Cert Log Cyl 00015F95  00017063 
 1st Decay    Cyl 00016001  000170CF 
 1st SPLASH   Cyl 0001601B  000170E9 
 Last System  Cyl 0001601C  000170EA 
T>
