

Test  : Data buffers reading (terminal)
Starting block........... : 0x0
Amount................... : 0x1F
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\U5\ST330621A-3.53-6EE04FEJ\Data\RAMDump\Data Buff 0x00000000 (0x0000001F).dmp
Result.................................. : Ok



Test  : RAM reading (by terminal)
Starting address......... : 0x0
Amount................... : 0x3F
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\U5\ST330621A-3.53-6EE04FEJ\Data\RAMDump\RAM 0x00000000 (0x0000003F).dmp
Result.................................. : Ok



Test  : ROM reading (terminal)
ROM file type............ : Programmator image
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!profiles\SeagateBara\U5\ST330621A-3.53-6EE04FEJ\Data\ROM\ROM.bin
Result.................................. : Error

Error reading Flash : RAM reading terminated by user

COM transfer baud rate setted to 57600


Test  : ROM reading (terminal)
ROM file type............ : Programmator image
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!profiles\SeagateBara\U5\ST330621A-3.53-6EE04FEJ\Data\ROM\ROM.bin
Result.................................. : Error

Error reading Flash : Terminal : error accepting data buffer data (Dump not full)

Terminal : Detecting SA bounds...
Trying to load CERT
Result.................................. : Ok
SA bounds defined


Test  : Reading SA surface by PCHS (terminal)
Location (PCHS).......... : 0x4304 : 0x0 : 0x0
Amount................... : 0x26D
HDD profile file......... : C:\Program Files\ACE Lab\PC-3000\Bin\!Profiles\SeagateBara\U5\ST330621A-3.53-6EE04FEJ\Data\PCHSDump\PCHS 0x004304_0x00_0x0000(0x026D).chs
Result.................................. : Error


Buffers reading terminated by user

Executing user command.................. : Show zones distribution

Executing user command.................. : Show Alt list (remap)

Executing user command.................. : Show User track slip list (P-List)

Executing user command.................. : Show Reserved track slip list

Executing user command.................. : Show PCB information

Executing user command.................. : Show buffers map

Executing user command.................. : Show ROM information

COM transfer baud rate setted to 9600

Executing user command.................. : Load CERT

Executing user command.................. : Switch HDD to ATA mode (Age=50)
