
(S) SATA Reset

(S) SATA Reset

(S) SATA Reset

ASCII Diag mode

F3 T>
ASCII Diag mode

 HighPowerMode 
TCC:001A
Status 0001 Req 0027
F3 T>/c

F3 C>Q

Online CR: Rev 0011.0000, Flash,   Abort
Online ESC: Rev 0011.0000, Flash,   Abort Looping Command or Batch File
Online ' ': Rev 0001.0000, Overlay, Pause Output
Online '.': Rev 0013.0000, Overlay, Display Active Status
Online '?': Rev 0011.0001, Overlay, Display Diagnostic Buffer Information
Online '`': Rev 0013.0000, Overlay, Display Read/Write Statistics
Online '$': Rev 0014.0000, Overlay, Display Read/Write Statistics By Zone
Online '': Rev 0011.0000, Overlay, Toggle EIB-Specific R/W Tracing
Online ^D: Rev 0011.0001, Overlay, Toggle R/W Tracing
Online ^N: Rev 0011.0001, Overlay, Toggle R/W Tracing
Online ^W: Rev 0011.0000, Overlay, Enable and Init RW Statistics
Online ^O: Rev 0003.0000, Overlay, Advance Servo Tracing State
Online ':': Rev 0001.0000, Overlay, PrepSecondaryOnlineCmd
Online '!': Rev 0011.0000, Overlay, Display Current Read Channel Settings
Online '<': Rev 0011.0000, Overlay, Decrement Read/Write Scope Sync
Online '>': Rev 0011.0000, Overlay, Increment Read/Write Scope Sync
Online '~': Rev 0015.0000, Overlay, Display Native Interface Command State
Online ^A: Rev 0018.0000, Flash,   Display Firmware Revision
Online ^B: Rev 0012.0000, Overlay, Get Thermistor Temperature
Online ^C: Rev 0011.0000, Overlay, Firmware Reset
Online ^E: Rev 0011.0000, Overlay, Display Native Interface Configuration
Online ^F: Rev 0011.0001, Overlay, Display Native Interface Read Cache Information
Online ^I: Rev 0011.0000, Overlay, Display Controller Registers
Online ^K: Rev 0011.0000, Overlay, Display DST Status
Online ^L: Rev 0021.0000, Overlay, Display Sign On Message
Online ^P: Rev 0011.0000, Overlay, Toggle Diag Idle Mode
Online ^Q: Rev 0011.0000, Overlay, Resume Interface Task
Online ^R: Rev 0011.0000, Flash,   Enable ASCII Online Serial Port Mode
Online ^S: Rev 0011.0000, Overlay, Pause Interface Task
Online ^T: Rev 0011.0000, Flash,   Enable ESLIP Serial Port Mode
Online ^U: Rev 0011.0000, Overlay, Display Congen
Online ^V: Rev 0011.0000, Overlay, Toggle Interface Command Echo
Online ^X: Rev 0012.0001, Overlay, Display Native Interface and Read/Write Command History
Online ^Y: Rev 0011.0000, Overlay, Display DST Status
Online ^Z: Rev 0011.0000, Flash,   Enable ASCII Diagnostic Serial Port Mode
Online ^\: Rev 0011.0000, Overlay, Toggle Debug Display Enable
Level : '`': Rev 0004.0000, Overlay, QMON Counters
Level : '$': Rev 0003.0000, Overlay, QMON Stats
Level : '@': Rev 0001.0000, Overlay, DRAM Refresh Intervals
Level : 'C'No help available
Level : 'E'No help available
Level : 'S'No help available
All Levels CR: Rev 0011.0000, Flash,   Abort
All Levels '/': Rev 0001.0000, Flash,   Change Diagnostic Command Level, /[Level]
All Levels '+': Rev 0012.0000, Flash,   Peek Memory Byte, +[AddrHi],[AddrLo],[NotUsed],[NumBytes]
All Levels '-': Rev 0012.0000, Flash,   Peek Memory Word, -[AddrHi],[AddrLo],[NotUsed],[NumBytes]
All Levels '=': Rev 0011.0002, Flash,   Poke Memory Byte, =[AddrHi],[AddrLo],[Data],[Opts]
All Levels 'A': Rev 0011.0001, Overlay, Set Test Space, A[OptsOrParmSelect],[ParmValue],[AddrType],[HdForCylLimit]
All Levels 'L': Rev 0001.0002, Overlay, Enable Looping, L[Opts],[CountOrStopOnErrCode]
Level 1 'N': Rev 0016.0001, Flash,   SMART Control, N[SubCmd],[SubCmdParm0],[SubCmdParm1]
Level 1 'B': Rev 0011.0000, Overlay, Buffer Display, B[DisplayBlk],[RefBlk],[NumBlks],[Opts],[SymBits]
Level 1 'D': Rev 0011.0001, Overlay, Memory Block Display, D[AddrHi],[AddrLo],[CompVal],[NumBytes],[Opts],[SizeInBytes]
Level 1 'G': Rev 0011.0000, Overlay, Generic Read/Write Request, G[Parm0],[Parm1],[Parm2],...[Parm9]
Level 1 'S': Rev 0011.0001, Overlay, Edit Processor Memory Byte, S[AddrHi],[AddrLo],[MemValue],[NumBytes],[Opts]
Level 1 'U': Rev 0011.0001, Overlay, Edit Buffer Memory Byte, U[AddrHi],[AddrLo],[MemValue],[NumBytes]
Level 1 'c': Rev 0011.0000, Overlay, Buffer Compare, c[SrcBlk],[RefBlk],[NumBlks],[ContOnErr]
Level 1 'e': Rev 0011.0000, Overlay, Spin Down and Reset Drive, e[MsecDelay],[Opts]
Level 1 'j': Rev 0001.0000, Overlay, Display Hardware Jumper Setting, j[HardwareJumperSelect]
Level 1 'm': Rev 0011.0001, Overlay, Edit Processor Memory Word, m[AddrHi],[AddrLo],[MemValue],[NumBytes],[Opts]
Level 1 's': Rev 0001.0000, Overlay, Call SDBP Cmd, s[Parm1],[Parm2],[Parm3]
Level 2 'x': Rev 0016.0000, Flash,   Display Zone Information, x[Partition],[Hd],[Zone],[Options]
Level 2 'B': Rev 0011.0000, Overlay, Buffer Display, B[DisplayBlk],[RefBlk],[NumBlks],[Opts],[SymBits]
Level 2 'C': Rev 0011.0000, Overlay, Buffer Copy, C[SrcBlk],[DestBlk],[NumBlks]
Level 2 'D': Rev 0001.0003, Overlay, LdpcIterationControl, D[itratn cnt],[glbl itratn],[BERP opts],[erasure],[slidewindowjog_sz],[ext itratn]
Level 2 'E': Rev 0015.0000, Overlay, Display / Edit Log, E[LogNum],[ErrCodeOrSpecialFuncKey],[SpecialFunc]
Level 2 'F': Rev 0011.0016, Overlay, Modify Track Defect List, F[PSctr/LBA],[Action]
Level 2 'H': Rev 0011.0000, Overlay, Select Logical Head, H[Hd],[SkType],[Options]
Level 2 'I': Rev 0016.0000, Overlay, Display / Modify Adaptive Parameter, I,[GroupId]
Level 2 'K': Rev 0011.0000, Overlay, Set Tracking Offset, K[OffsetValue],[PersOrTempOpt],[UnitsOpt],[ChanReload]
Level 2 'M': Rev 0012.0000, Overlay, Set Diag Idle Mode, M[ModeSelect],[ModeMask],[ResetToPowerOn]
Level 2 'N': Rev 0001.0000, Overlay, Set Direct Write Mode, N[EnableDirWrtModeOpt]
Level 2 'O': Rev 0011.0000, Overlay, Seek Repeatedly Between Physical Cylinders, O[StartPhyCyl0],[StartPhyCyl1],[NumSkPairs],[NumSeconds],[Hd]
Level 2 'P': Rev 0011.0000, Overlay, Set Buffer Pattern, P[PatternSelOrPatternLow],[PatternHi],[PatternBits],[Opts],[BlkNum],[NumBlks]
Level 2 'Q': Rev 0011.0001, Overlay, Write, Read, Read CHS, Q[Sec],[NumSecs],,[PhyOpt],[Opts]
Level 2 'R': Rev 0011.0003, Overlay, Read CHS, R[Sec],[NumSecs],,[PhyOpt],[Opts]
Level 2 'S': Rev 0011.0000, Overlay, Seek to Logical Cylinder and Head, S[Cyl],[Hd],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 2 'T': Rev 0015.0000, Overlay, Measure Throughput, T[Opts],[CylSkew],[HeadSkew],[MiniZoneSkew],[SkewStep],[LengthInTracks],[OffsetInTracks],[NumberOfRetries]
Level 2 'U': Rev 0011.0000, Overlay, Spin Up Drive, U[HoldState],[Hd],[Cyl]
Level 2 'V': Rev 0011.0001, Overlay, Read Verify CHS, V[Sec],[NumSecs],[CompareBlk],[Opts]
Level 2 'W': Rev 0011.0002, Overlay, Write CHS, W[Sec],[NumSecs],,[PhyOpt],[Opts]
Level 2 'X': Rev 0015.0001, Overlay, Display Track Information, X[LogCyl],[Hd],[SysAreaOpt],[Opts],[RowsPerPage]
Level 2 'Y': Rev 0012.0000, Overlay, Set Retries - DERP, Y[Mode],[MaxRdRetries],[MaxWrtRetries],[OtcTLevel],[Options]
Level 2 'Z': Rev 0011.0000, Overlay, Spin Down Drive, Z
Level 2 'a': Rev 0002.0000, Overlay, Measure Optimum Skew, a
Level 2 'b': Rev 0002.0000, Overlay, BER by Hd / Zone, b[hd][,zone]
Level 2 'c': Rev 0011.0000, Overlay, Buffer Compare, c[SrcBlk],[RefBlk],[NumBlks],[ContOnErr]
Level 2 'h': Rev 0015.0000, Overlay, Translate Physical Sector, h[Sec],[NumSecs]
Level 2 'i': Rev 0011.0000, Overlay, Display Defects On Current Track, i[Print Summary]
Level 2 'j': Rev 0011.0001, Overlay, Read Wedge, j[WedgeAddr],[NumWedges],[NumSkipedWedges],[TranSize],[Opts],[RegAddr0],...,[RegAddr13]
Level 2 'k': Rev 0001.0000, Overlay, Set User Cylinder/Head/MiniZone Skew, k[CylSkew],[HeadSkew],[MiniZoneSkew]
Level 2 'l': Rev 0015.0000, Overlay, Translate Logical Sector, l[Sec],[NumSecs]
Level 2 'o': Rev 0002.0001, Overlay, Corrupt LBA, o[Lba],[NumBlocks],[BurstSpan],[BurstOffset],[NumberOfRandomCorrupt],[Flags]
Level 2 'r': Rev 0011.0001, Overlay, Read Long CHS or Read System CHS, r[LongSec],[LongSecsOrSysSec],[SysSecs],[LongPhySecOpt],[LongOpts],[SysOpts]
Level 2 's': Rev 0011.0000, Overlay, Seek to Physical Cylinder and Head, s[Cyl],[Hd],[ValidKey],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 2 't': Rev 0015.0000, Overlay, Translate Wedge, t[Wdg],[NumWdgs]
Level 2 'u': Rev 0011.0000, Overlay, Enable/Disable Channel/Preamp Register Display, u[EnableDisableOpt]
Level 2 'v': Rev 0011.0000, Overlay, Convert Data Track Percentage To Servo Offset Count, v[Percentage]
Level 2 'w': Rev 0012.0001, Overlay, Write Long CHS or Write System CHS, w[LongSec],[LongSecsOrSysSec],[SysSecs],[LongPhySecOpt],,[SysOpts]
Level 2 'y': Rev 0011.0000, Overlay, Set DERP Retry State, y[Type],[PathState],[RetryStateCnt],[LoopCnt1],[LoopCnt2]
Level 2 'z': Rev 0011.0002, Overlay, Write Wedge, z[WedgeAddr],[NumWedges],[NumSkipedWedges],[TranSize],[Opt],[RegAddr0],...,[RegAddr13],[TSpacing]
Level 2 '7': Rev 0011.0001, Overlay, Write Verify CHS, 7[Sec],[NumSecs],[WrBufBlk],[Opts]
Level 3 'D': Rev 0011.0000, Overlay, Measure Seek Access Time, D[SkLength],[SkType],[NumSks]
Level 3 'E': Rev 0015.0000, Overlay, Display / Edit Log, E[LogNum],[ErrCodeOrSpecialFuncKey],[SpecialFunc]
Level 3 'H': Rev 0011.0000, Overlay, Select Logical Head, H[Hd],[SkType],[Options]
Level 3 'O': Rev 0011.0000, Overlay, Seek Repeatedly Between Physical Cylinders, O[StartPhyCyl0],[StartPhyCyl1],[NumSkPairs],[NumSeconds],[Hd]
Level 3 'Q': Rev 0011.0001, Overlay, Write, Read, Write, Read CHS, Q[Sec],[NumSecs],[Opts]
Level 3 'R': Rev 0011.0000, Overlay, Read Current Servo Destination, R
Level 3 'S': Rev 0011.0000, Overlay, Seek to Logical Cylinder and Head, S[Cyl],[Hd],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 3 'U': Rev 0011.0000, Overlay, Spin Up Drive, U[HoldState],[Hd],[Cyl]
Level 3 'V': Rev 0012.0000, Overlay, Read or Write Power ASIC Register, V[RegAddr],[RegValue],[WrOpt]
Level 3 'Z': Rev 0011.0000, Overlay, Spin Down Drive, Z
Level 3 'b': Rev 0001.0000, Overlay, LoadUnloadHeads, b[Cmd],[Velocity],[Dwell],[Lock]
Level 3 'f': Rev 0013.0000, Overlay, Real Time Servo Trace, f[SubCmd],[SubPrm0],[SubPrm1],[SubPrm2]
Level 3 'p': Rev 0015.0000, Overlay, Translate Physical Sector, p[Sec],[NumSecs]
Level 3 'q': Rev 0015.0000, Overlay, Translate Logical Sector, q[Sec],[NumSecs]
Level 3 's': Rev 0011.0000, Overlay, Seek to Physical Cylinder and Head, s[Cyl],[Hd],[ValidKey],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 4 'B': Rev 0011.0000, Overlay, Enable / Disable RVFF, B[NewRvffControlMode]
Level 4 'D': Rev 0011.0000, Overlay, Measure Seek Access Time, D[SkLength],[SkType],[NumSks]
Level 4 'E': Rev 0015.0000, Overlay, Display / Edit Log, E[LogNum],[ErrCodeOrSpecialFuncKey],[SpecialFunc]
Level 4 'F': Rev 0001.0000, Overlay, Fast IO Cmd, F[NumRevs],[Attrib1],[Attrib2],[Attrib3]
Level 4 'H': Rev 0011.0000, Overlay, Select Logical Head, H[Hd],[SkType],[Options]
Level 4 'K': Rev 0011.0000, Overlay, Set Tracking Offset, K[OffsetValue],[PersOrTempOpt],[UnitsOpt],[ChanReload]
Level 4 'O': Rev 0011.0000, Overlay, Display Micro Jog for Logical Cylinder and Head, O[LogCyl],[Hd],[Opts],[SysAreaOpt]
Level 4 'S': Rev 0011.0000, Overlay, Seek to Logical Cylinder and Head, S[Cyl],[Hd],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 4 'U': Rev 0011.0000, Overlay, Servo Batch Test sub commands, U[SubCmd],[SubCmdParm0],[SubCmdParm1],[SubCmdParm2]
Level 4 'c': Rev 0001.0000, Overlay, Find Min Or Max Cylinders c[Head],[Mode],[RangeMultiplier],[RetryCountLimit],[FilterTimeConstant]
Level 4 'd': Rev 0001.0000, Overlay, Display Servo Disc Slip
Level 4 'e': Rev 0011.0000, Overlay, Enable / Disable PES Output, e[PesLeftShiftCnt],[DisablePesOut]
Level 4 'g': Rev 0001.0000, Overlay, Display Servo Sector Error Log, g
Level 4 'k': Rev 0001.0000, Overlay, Get VGA Data, k[OpType],[StartHt],[EndHt],[HtInc]
Level 4 'l': Rev 0011.0000, Overlay, Scan Track for Servo Defects and ZAP, l[RdPositionOpt]
Level 4 'q': Rev 0001.0000, Overlay, Display Servo Event Log, q
Level 4 's': Rev 0001.0000, Overlay, Display Servo Sector Error Count, s
Level 4 't': Rev 0011.0000, Overlay, Display / Modify ZAP Table, t[EntryNum],[EntryValue]
Level 4 'u': Rev 0011.0000, Overlay, Set Seek Speed, u[Opts],[SkSpeed]
Level 4 'v': Rev 0011.0000, Overlay, Butterfly Seek Test, v[StartPhyCyl0],[StartPhyCyl1],[NumSkPairs],[NumSeconds],[Hd]
Level 5 'E': Rev 0001.0000, Flash,   Measure Disc Eccentricity
Level 5 'R': Rev 0011.0000, Flash,   Read Servo RAM at Address, R[Addr],[NumBytes]
Level 5 'S': Rev 0011.0000, Flash,   Enter Servo Matlab Shell, S
Level 5 'B': Rev 0011.0000, Overlay, Servo Bode Plot, B[BodeType],[InjAmp],[Fmin],[Fmax],[NumFreq],[NumSamples],[EnableTracing]
Level 5 'C': Rev 0011.0000, Overlay, Generic Servo Command, C[CmdNum],[Parm1],...[Parm7]
Level 5 'D': Rev 0011.0000, Overlay, Read / Unlock DDR Buffer, B[OperateCode]
Level 5 'F': Rev 0011.0001, Overlay, DriveFreeFallProtection, F[OpCode],[FreeFallSen],[TumbleSen],[SimDur],[SimSensorOutputs]
Level 5 'G': Rev 0011.0000, Overlay, Select Servo Controller, G[Head],[Controller],[InputShift]
Level 5 'K': Rev 0001.0000, Overlay, Servo Disc Slip, K [OperationSelectId]
Level 5 'U': Rev 0011.0000, Overlay, Enable / Disable Servo Updates, U[VcmDacUpdateOpt],[AToDUdateOpt]
Level 5 'W': Rev 0011.0000, Overlay, Write Servo RAM at Address, W[Addr],[NumBytes],[Data]
Level 5 'Z': Rev 0011.0000, Overlay, Read Zap from Disc to Table, Z
Level 5 'd': Rev 0011.0000, Overlay, Disable / Enable Servo ZAP coefficients and ZAP read, d[ZapControlMode]
Level 5 'e': Rev 0001.0000, Overlay, Enable / Disable Shock Sensor, e[Operation]
Level 5 'i': Rev 0011.0000, Overlay, Read Servo Symbol Table at Index, i[Index]
Level 5 'p': Rev 0001.0000, Overlay, Set Power Mode, p[PowerMode]
Level 5 'r': Rev 0011.0000, Overlay, Read Servo RAM at Index, r[Index],[NumBytes],[ByteOffset]
Level 5 'w': Rev 0011.0000, Overlay, Write Servo RAM at Index, w[Index],[NumBytes],[Data],[ByteOffset]
Level 7 'x': Rev 0016.0000, Flash,   Display Zone Information, x[Partition],[Hd],[Zone],[Options]
Level 7 'B': Rev 0011.0000, Overlay, Buffer Display, B[DisplayBlk],[RefBlk],[NumBlks],[Opts],[SymBits]
Level 7 'C': Rev 0011.0000, Overlay, Buffer Copy, C[SrcBlk],[DestBlk],[NumBlks]
Level 7 'D': Rev 0012.0000, Overlay, Display Temperature, D,[DevSelect]
Level 7 'E': Rev 0015.0000, Overlay, Display / Edit Log, E[LogNum],[ErrCodeOrSpecialFuncKey],[SpecialFunc]
Level 7 'H': Rev 0011.0000, Overlay, Select Logical Head, H[Hd],[SkType],[Options]
Level 7 'I': Rev 0016.0000, Overlay, Display / Modify Adaptive Parameter, I,[GroupId]
Level 7 'K': Rev 0011.0000, Overlay, Set Track Format, K[UserAreaTrkFormatType],[SysAreaTrkFormatType]
Level 7 'P': Rev 0011.0000, Overlay, Set Buffer Pattern, P[PatternSelOrPatternLow],[PatternHi],[PatternBits],[Opts],[BlkNum],[NumBlks]
Level 7 'Q': Rev 0011.0001, Overlay, Write, Read, Read CHS, Q[Sec],[NumSecs],,[PhyOpt],[Opts]
Level 7 'R': Rev 0011.0003, Overlay, Read CHS, R[Sec],[NumSecs],,[PhyOpt],[Opts]
Level 7 'S': Rev 0011.0000, Overlay, Seek to Logical Cylinder and Head, S[Cyl],[Hd],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 7 'U': Rev 0015.0005, Overlay, Preamp Temperature Adjust, U[TweakTemperature],[Partition],[Hd],[Zone],[Opts],[WrPreht],[WrWrtHt],[WrRdHt],[RdPreht],[RdWrtHt],[RdRdHt],[RelHum]
Level 7 'W': Rev 0011.0002, Overlay, Write CHS, W[Sec],[NumSecs],,[PhyOpt],[Opts]
Level 7 'X': Rev 0011.0000, Overlay, Display Preamp Head Resistance
Level 7 'Y': Rev 0012.0000, Overlay, Set Retries - DERP, Y[Mode],[MaxRdRetries],[MaxWrtRetries],[OtcTLevel],[Options]
Level 7 'Z': Rev 0011.0000, Overlay, Spin Down Drive, Z
Level 7 'b': Rev 0012.0000, Overlay, Erase Track, b[AdjacentTrkCnt],[EraseCntPerTrk],[AcEraseOpt]
Level 7 'c': Rev 0011.0000, Overlay, Off Track Capability, c[Sec],[NumSecs],[SecIncrement],[Offset]
Level 7 'd': Rev 0002.0000, Overlay, Create Recoverable Read Error, d LBA,[min],[max],[cnt],[sev]
Level 7 'e': Rev 0001.0000, Overlay, BipsControl, e[BipsControlOptions]
Level 7 'g': Rev 0001.0000, Overlay, Sector Based BER, g[sctr],[len],[option]
Level 7 'h': Rev 0011.0001, Overlay, Mark Media Flaw, h[PhyCyl],[Hd],[PhySec],[UndisturbedRadius],[EraseBandTrks],[PtrLen],[WgSpec],[Od/Id]
Level 7 'i': Rev 0011.0000, Overlay, Generic Read/Write Request, i[Parm0],[Parm1],[Parm2],...[Parm9]
Level 7 'm': Rev 0025.0000, Overlay, Display DOS Information, m[Flags],[LBA],[MinCnt]
Level 7 'p': Rev 0002.0000, Overlay, Execute Pressure Sensor Command, p[SubCmd]
Level 7 'r': Rev 0011.0000, Overlay, Read Non-Volatile Adaptive Parameters, r[Opts]
Level 7 's': Rev 0011.0000, Overlay, Write Peripheral Register - channel or preamp, s[OpType],[RegAddr],[RegValue],[RegMask],[RegPagAddr]
Level 7 't': Rev 0012.0000, Overlay, Read Peripheral Register - channel or preamp, t[OpType],[RegAddr],[NumRegs],[RegMask],[RegPagAddr]
Level 7 'u': Rev 0011.0000, Overlay, Enable/Disable Write Fault, u[Op]
Level 7 'w': Rev 0011.0000, Overlay, Save Adaptives To Flash, w[Seg],,22
Level 7 'y': Rev 0011.0000, Overlay, Set DERP Retry State, y[Type],[PathState],[RetryStateCnt],[LoopCnt1],[LoopCnt2]
Level 8 'C': Rev 0011.0000, Overlay, Servo Diag Sub Cmds, C[SubCmd],[Parm0],[Parm1],[Parm2]
Level 8 'R': Rev 0011.0000, Overlay, Read Current Servo Destination, R
Level 8 'S': Rev 0011.0000, Overlay, Seek to Logical Cylinder and Head, S[Cyl],[Hd],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level 8 'U': Rev 0011.0000, Overlay, Spin Up Drive, U[HoldState],[Hd],[Cyl]
Level 8 'Z': Rev 0011.0000, Overlay, Spin Down Drive, Z
Level 8 'd': Rev 0001.0000, Overlay, Head Smash Test, d[HeadDirection],[AccelerationDuration],[DecelerationDuration],[AccelerationCurrent],[DecelerationCurrent]
Level A 'C': Rev 0015.0000, Overlay, Translate PBA, C[PbaHi],[PbaLow],[NumPbas]
Level A 'D': Rev 0015.0000, Overlay, Translate Symbols From Index, D[PhyCyl],[Hd],[Sfi],[NumSfis]
Level A 'E': Rev 0015.0000, Overlay, Display / Edit Log, E[LogNum],[ErrCodeOrSpecialFuncKey],[SpecialFunc]
Level A 'F': Rev 0015.0001, Overlay, Translate LBA, F[LbaHi],[LbaLo],[SysAreaOpt],[NumLbas]
Level A 'G': Rev 0015.0000, Overlay, Translate Host LBA, T[LbaHi],[LbaLo],[NumLbas]
Level A 'M': Rev 0011.0000, Overlay, Set Controller Test Port, M[Port],[Value]
Level A 'P': Rev 0013.0001, Overlay, Merge Alt List into Slip List, P[RADIAL_PAD_IN_TRACKS],[CIRCUMFERENTIAL_PAD_SINGLE_IN_WEDGES],[CIRCUMFERENTIAL_PAD_MULTI_IN_WEDGES],[OPTIONS]
Level A 'Q': Rev 0011.0001, Overlay, Write, Read, Read LBA, Q[Lba],[NumLbas],[Opts]
Level A 'R': Rev 0011.0003, Overlay, Read LBA, R[Lba],[NumLbas],,[Opts]
Level A 'S': Rev 0011.0000, Overlay, Seek to LBA, S[LbaHi],[LbaLo],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level A 'T': Rev 0001.0000, Overlay, GetLbaTracks, T[Zone],[Head]
Level A 'W': Rev 0011.0002, Overlay, Write LBA, W[Lba],[NumLbas],,[Opts]
Level A 'Y': Rev 0012.0000, Overlay, Set Retries - DERP, Y[Mode],[MaxRdRetries],[MaxWrtRetries],[OtcTLevel],[Options]
Level A 'c': Rev 0015.0000, Overlay, Translate Logical Cylinder, Logical Head and Logical Sector, c[Cyl],[Hd],[Sec],[SysAreaOpt],[NumSecs]
Level A 'd': Rev 0015.0000, Overlay, Translate Physical Cylinder, Logical Head and Physical Sector, d[Cyl],[Hd],[Sec],[NumSecs]
Level A 'e': Rev 0015.0000, Overlay, Translate Nominal Cylinder and Logical Head, e[Cyl],[Hd],[Sec],[SysAreaOpt]
Level A 'f': Rev 0015.0000, Overlay, Translate Physical Cylinder, Logical Head and Physical Wedge, f[Cyl],[Hd],[Wdg],[NumWdgs]
Level A 'l': Rev 0015.0001, Overlay, Display Track Information, l[LogCyl],[Hd],[SysAreaOpt],[Opts],[RowsPerPage]
Level A 'y': Rev 0011.0000, Overlay, Set DERP Retry State, y[Type],[PathState],[RetryStateCnt],[LoopCnt1],[LoopCnt2]
Level C 'B': Rev 0001.0001, Overlay, Display Channel Status List Data
Level C 'C': Rev 0001.0000, Overlay, Display Select Channel Register, C[ChannelRegAsciiString]
Level C 'D': Rev 0003.0000, Overlay, Display Bonanza Memory, D[MemorySelect],[StartAddress],[NumberOfSymbols],[BufferSelect]
Level C 'E': Rev 0001.0000, Overlay, Display Bonanza Memory Size, E
Level C 'G': Rev 0001.0000, Overlay, Set Channel Status List Triggers,[mask]
Level C 'H': Rev 0001.0000, Overlay, Set Channel Status List Thresholds,[action],[value]
Level C 'Q': Rev 0001.0000, Overlay, Display ASCII Command Information, Q[CmdLevel],[Cmd]
Level C 'S': Rev 0000.0000, Overlay, Display Channel Status List Status
Level C 'T': Rev 0012.0000, Overlay, Goop Plot, T[Hd],[StartTrk],[EndTrk],[ECCLvl],[NoFrcSync],[SkipCnt]
Level E 'B': Rev 0011.0002, Overlay, Write Wedge, B[WedgeAddr],[NumWedges],[NumSkipedWedges],[TranSize],[Opt],[RegAddr0],...,[RegAddr13],[TSpacing]
Level E 'C': Rev 0011.0001, Overlay, Read Wedge, C[WedgeAddr],[NumWedges],[NumSkipedWedges],[TranSize],[Opts],[RegAddr0],...,[RegAddr13]
Level E 'G': Rev 0001.0000, Overlay, HeadDegradation, G[OperationControlOptions],[MeasurementControlOptions]
Level E 'm': Rev 0011.0000, Overlay, Fast MSESER Measurement, m[]
Level E 'n': Rev 0001.0000, Overlay, Dibit Extraction, n[sctr],[cnt],[dibit],[dibit],[dibit],[skip],[trim],[dsply]
Level E 'o': Rev 0011.0000, Overlay, Fine RW Offset Measurement, o[NumAvgs],[TrkStepSize],[NumGuardTrks]
Level E 'w': Rev 0011.0002, Overlay, Slow Write CHS, w[Sec],[NumSecs],[ConSec],[Skip],[UnitOfSkip]
Level F 'b': Rev 0011.0000, Flash,   Set Baud Rate, b[BaudRate],[MsecDelay]
Level F 'B': Rev 0011.0000, Overlay, Buffer Display, B[DisplayBlk],[RefBlk],[NumBlks],[Opts],[SymBits]
Level F 'C': Rev 0011.0000, Overlay, Buffer Copy, C[SrcBlk],[DestBlk],[NumBlks]
Level F 'D': Rev 0011.0001, Overlay, Memory Block Display, D[AddrHi],[AddrLo],[CompVal],[NumBytes],[Opts],[SizeInBytes]
Level F 'P': Rev 0011.0000, Overlay, Set Buffer Pattern, P[PatternSelOrPatternLow],[PatternHi],[PatternBits],[Opts],[BlkNum],[NumBlks]
Level F 'U': Rev 0011.0000, Overlay, Spin Up Drive, U[HoldState],[Hd],[Cyl]
Level F 'V': Rev 0011.0000, Overlay, Buffer Compare, V[SrcBlk],[RefBlk],[NumBlks],[ContOnErr]
Level F 'Y': Rev 0012.0000, Overlay, Set Retries - DERP, Y[Mode],[MaxRdRetries],[MaxWrtRetries],[OtcTLevel],[Options]
Level F 'Z': Rev 0011.0000, Overlay, Spin Down Drive, Z
Level F 'r': Rev 0011.0001, Overlay, Read System CHS, r[LogSec],[NumSecs],[Opts]
Level F 's': Rev 0011.0000, Overlay, Seek to Physical Cylinder and Head, s[Cyl],[Hd],[ValidKey],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level F 't': Rev 0011.0000, Overlay, Write Peripheral Register - channel or preamp, t[OpType],[RegAddr],[RegValue],[RegMask],[RegPagAddr]
Level F 'y': Rev 0011.0000, Overlay, Set DERP Retry State, y[Type],[PathState],[RetryStateCnt],[LoopCnt1],[LoopCnt2]
Level F 'z': Rev 0011.0000, Overlay, SataDebug, z[SubCmd],[Parm1],[Parm2],[Parm3]
Level G 'B': Rev 0011.0000, Overlay, Fill Correction Buffer, B[StartAddr],[EndAddr],[Pattern],[Opts]
Level G 'C': Rev 0011.0000, Overlay, Copy Correction Buffer, C[SrcAddr],[DestAddr],[NumSyms]
Level G 'D': Rev 0011.0000, Overlay, Display Correction Buffer, D[StartAddr],[EndAddr],[CompareData]
Level G 'F': Rev 0011.0000, Overlay, Fill Super Parity RAM, F[StartAddr],[EndAddr],[Pattern]
Level G 'G': Rev 0011.0000, Overlay, Display Super Parity RAM, G[StartAddr],[EndAddr]
Level H 'B': Rev 0011.0000, Overlay, Buffer Display, B[DisplayBlk],[RefBlk],[NumBlks],[Opts],[SymBits]
Level H 'I': Rev 0001.0000, Overlay, Serial Identify, I[Strt],[Cnt]
Level H 'P': Rev 0011.0000, Overlay, Set Buffer Pattern, P[PatternSelOrPatternLow],[PatternHi],[PatternBits],[Opts],[BlkNum],[NumBlks]
Level H 'S': Rev 0011.0000, Overlay, Seek to Logical Cylinder and Head, S[Cyl],[Hd],[Offset],[OffsetUnitsOpt],[SkType],[Options]
Level H 'b': Rev 0013.0001, Overlay, Contact Detect, b[Flags],[Revs],[BaselineRevs],[StartWedge],[A],[B],[C],[D],[E],[StartHt],[HtInc],
[FixedPESThresh],[FilterDelta],[RangeStart],[RangePts],[AdjThreshSigmaLimit],[VarContactThreshBackup],[InactiveHt]
Level L 'C': Rev 0011.0000, Overlay, Copy Log File, C[SrcLog],[DestLog],[AppendOpt]
Level L 'D': Rev 0013.0000, Overlay, Display Log File, D[Log],[ErrCode]
Level L 'E': Rev 0011.0001, Overlay, Enable / Disable Logging, E[ErrLoggingOpt],[AsciiLoggingOpt],[RwStatsLoggingOpt]
Level L 'I': Rev 0011.0000, Overlay, Display Log FileInfo, I[Log]
Level L 'c': Rev 0011.0000, Overlay, Create Log File, c[Log],[LogType],[BufferOrDiskOpt],[NumBytes]
Level L 'd': Rev 0011.0000, Overlay, Delete Log File, d[Log]
Level L 'i': Rev 0011.0000, Overlay, Initialize Log File, i[Log]
Level M 's': Rev 0001.0000, Overlay, Serial Port Test Results, s[Sub-command],[SptIndex],[ValidKey]
Level N 'B': Rev 0001.0000, Overlay, NvcManageBadClumps, B[SubCommand]
Level N 'C': Rev 0001.0000, Overlay, NvcCopyClumps, C[SubCommand],[SrcClump],[SrcClumpOffset],[DestClump],[DestClumpOffset],[LBA],[SecLength]0 - User data copy1 - System data copy
Level N 'd': Rev 0002.0001, Overlay, NvcDumpFlashMetadata, d[SubCommand],[Clump],[BlockOffset],[Count] 0=Linear Order,[ForceComboMode]
Level N 'E': Rev 0002.0000, Overlay, NvcEraseFlash, E[SubCommand],[StartClump],[ClumpCount],[ForceErase] Note, E[SubCommand],DEADBEEF == Erase all
Level N 'G': Rev 0001.0000, Overlay, NvcReadWriteLong, G[SubCommand],[LBA],[#BitsToFlip],[StartAddr]
Level N 'h': Rev 0001.0000, Overlay, NvcPrintPsmCmdHistory, h
Level N 'I': Rev 0001.0000, Overlay, NvcInitializeFlashIODriver, I[InitializationComponent]
Level N 'm': Rev 0001.0000, Overlay, NvcDisplayMemory, m[MemoryArea],[Offset],[Options]0-Unused1-Reserved2-FlashDataManager3-word4-sector by byte offset5-sector by sector offset6-Capilano word7-Capilano 128 words
Level N 'M': Rev 0001.0000, Overlay, NvcModifyMemory, M[MemoryArea],[Offset],[Value],[Options]
Level N 'r': Rev 0001.0000, Overlay, NvcReadFlashData, r[SubCommand],[Clump],[BlockOffset],[BlockCount],[TargetAddress],[LBA]0-TargetAddress is iRAM sector1-TargetAddress is any VBM
Level N 'V': Rev 0001.0000, Overlay, NvcFlashVerificationTest, V[SubCommand],[StartClump],[ClumpCount],[StartBlock],[BlockCount],[Pattern],[PatternOptions],[TotalLoopCount],[ReadLoopCount]
Level N 'v': Rev 0001.0000, Overlay, Display NVC Hardware Info, v
Level N 'W': Rev 0001.0000, Overlay, NvcWriteFlashData, W[SubCommand],[Clump],[BlockOffset],[BlockCount],[TargetAddress],[LBA]0-TargetAddress is iRAM sector1-TargetAddress is any VBM
Level O 'a': Rev 0001.0000, Overlay, CfsReturnActiveClump, a[ClumpDataType]
Level O 'b': Rev 0002.0000, Overlay, CfsConciseReliDisplayCmd, b0
Level O 'c': Rev 0004.0000, Overlay, CfsReturnClumpNode, c[SubCommand],[ClumpIndex]
Level O 'C': Rev 0002.0000, Overlay, CfsDisplayClumpList, C[ClumpList]
Level O 'G': Rev 0001.0000, Overlay, ReadWriteLong, G[SubCommand],[DataType],[StartLba],[EndLba]
Level O 'I': Rev 0001.0000, Overlay, CfsInitializeCacheFileSystem, I
Level O 'j': Rev 0001.0000, Overlay, CfsPrintAsdJournal, j0
Level O 'K': Rev 0001.0000, Overlay, CopyClumpsCmd, K[source]
Level O 'l': Rev 0001.0000, Overlay, CfsLoadCacheFileSystem, l
Level O 'n': Rev 0002.0000, Overlay, CfsReturnCacheNode, n[NodeIndex]
Level O 'p': Rev 0001.0000, Overlay, CfsDisplayClumpForIndex, p[NodeIndex]
Level O 'r': Rev 0001.0000, Overlay, CfsReadNodeLba, r[StartLBA],[Count] Currently this command is not functional
Level O 's': Rev 0001.0000, Overlay, CfsDisplaySentinelList, s[SentinelIndex],[StartLBA],[EndLBA]
Level O 'S': Rev 0001.0000, Overlay, CfsSaveCacheFileSystem, S
Level O 'v': Rev 0001.0003, Overlay, CfsVerifyIntegrity, v[TestSelection]
Level T 'B': Rev 0011.0000, Flash,   Set Baud Rate, B[BaudRate],[MsecDelay]
Level T 'S': Rev 0001.0000, Flash,   Reset drive customer settings, SHIP,[ParmValue]
Level T 'V': Rev 0027.0000, Flash,   Display Defect Lists, V[ListMask],[Hd],[StartCyl],[NumCyls],[Summary],[FlagsMask]
Level T 'E': Rev 0015.0000, Overlay, Display / Edit Log, E[LogNum],[ErrCodeOrSpecialFuncKey],[SpecialFunc]
Level T 'F': Rev 0011.0000, Overlay, Display / Modify Congen, F[ValueRef],[Data],[ResetEnable]
Level T 'J': Rev 0011.0001, Overlay, Display / Modify CAP, J[ParmValue],[ParmId],[ParmArrayBytes],[ParmByteArrayOffset]
Level T 'O': Rev 0001.0000, Overlay, Select Data Output Mode, O[Mode],[VerboseOpts]
Level T 'P': Rev 0011.0000, Overlay, Download Generic File, P[FileBytes]
Level T 'R': Rev 0011.0000, Overlay, Read Non-Volatile Adaptive Parameters, R[Opts]
Level T 'W': Rev 0011.0000, Overlay, Save Adaptives To Flash, W[Seg],,22
Level T 'i': Rev 0011.0003, Overlay, Initialize Defect List, i[DefectListSelect],[SaveListOpt],[ValidKey]
Level T 'm': Rev 0015.0067, Overlay, Format Partition, m[Partition],[FormatOpts],[DefectListOpts],[MaxWrRetryCnt],[MaxRdRetryCnt],[MaxEccTLevel],[MaxCertifyTrkRewrites],[ValidKey],[DataPattern]
Level T 'r': Rev 0001.0000, Overlay, Read File, r[FileId],[VolumeNum],[CopyNum],[ByteOffset],[Length],[OutputFmt]
Level T 'q': Rev 0001.0000, Overlay, List Physical Head Table, q
Level T 'w': Rev 0001.0000, Overlay, Write File, w[FileId],[VolumeNum],[CopyNum],[ByteOffset]
Level T 'y': Rev 0001.0000, Overlay, List SIM files, y[Volume], [FileDescriptor]
Level T '[': Rev 0011.0000, Overlay, ASCII Log Control, [[LogFunction],[Log]
F3 C>
