Vendor identification : CSD
Product identification : CSM036
Product revision level :
Peripheral Qualifier : Device is connected to this LUN
Device type : Direct-access device (magnetic disk)
Removable medium : No
Compliance to the ISO version of SCSI : No
Compliance to the ECMA version of SCSI : No
ANSI-approved version : ANSI X3.301-1997
Asynchronous event notification capability : Not supported
Terminate I/O process : Not supported
Data format : 2
Additional length : 91
Relative Addressing : Not supported
32-bit Wide data Xfer : Not supported
16-bit Wide data Xfer : Supported
Synchronous data transfer : Supported
Linked commands : Supported
Tagged command queuing : Supported
Soft reset : Not supported
32-bit wide SCSI addresses : Not supported
16-bit wide SCSI addresses : Supported
Continue I/O Process and Target Transfer Disable messages : Supported

 Vital Product Information
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴
Page 80h - Unit Serial Number Page
  Serial Number:

Page C0h - Firmware Numbers Page
  0A C0 00 00

Disk 34.2GB 71770616/512 15000rpm Bfr=7MB
