Vendor identification : FUJITSU 
Product identification : MAB3045SP       
Product revision level : 0109    
Peripheral Qualifier : Device is connected to this LUN
Device type : Direct-access device (magnetic disk)
Removable medium : No
Compliance to the ISO version of SCSI : No
Compliance to the ECMA version of SCSI : No
ANSI-approved version : ANSI X3.131-1994 (SCSI-2)
Asynchronous event notification capability : Not supported
Terminate I/O process : Supported
Data format : 2  
Additional length : 59
Relative Addressing : Not supported
32-bit Wide data Xfer : Not supported
16-bit Wide data Xfer : Supported
Synchronous data transfer : Supported
Linked commands : Supported
Tagged command queuing : Supported
Soft reset : Not supported
32-bit wide SCSI addresses : Not supported
16-bit wide SCSI addresses : Supported
Continue I/O Process and Target Transfer Disable messages : Supported
